**Remove and Replace existing security gates at Troop F**

**Location:**

Louisiana State Police-Troop F

1240 Highway 594

Monroe, LA 71203

**Scope of Work:**

Contractor shall furnish all materials, equipment, tools and labor needed to remove two existing security gates and replace with two new security gates at Troop F. Contractor shall also tie into existing open/close switch that is located at the front desk area of the Troop F.

**Requirements:**

* Contractor shall remove the two existing security gates used as entrance and exit to a secured area into the Troop F facility and replace with new gates.
* Contractor shall install two 35 feet cantilever chain-link fence gates with a minimum of six vertical braces per gate, with appropriate counter weight bracing throughout the gates as required.
* Each gate shall have a total of eight, 3 inch nylon top and bottom cantilever rollers (four top and four on bottom).
* The gates shall be at least 5 1/2 feet tall plus three strands of security barb wire that total 16 inches above the top of gate.
* Contractor shall install two HDSL, 24 UL Liftmaster slide gate commercial grade motors, or equal.
	+ If not bidding as specified, please indicate Make/Model bidding:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + Contractor shall install one Liftmaster universal wireless entry keypad, or equal.
	+ If not bidding as specified, please indicate Make/Model bidding:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + Contractor shall install two MMTC Omron reflective photo eyes, or equal.
	+ If not bidding as specified, please indicate Make/Model bidding:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + Contractor shall install one Eagle EFB 2070 emergency fire access box, or equal.
	+ If not bidding as specified, please indicate Make/Model bidding:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + Contractor shall install one Liftmaster wireless exit loop for exit gate, or equal.
	+ If not bidding as specified, please indicate Make/Model bidding:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + Contractor shall install three Liftmaster (LOOPDETLM-model) safety loops for both gates, or equal.
	+ If not bidding as specified, please indicate Make/Model bidding:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + Contractor shall install four Liftmaster (LOOPDETLM-model) loop detectors, or equal.
	+ If not bidding as specified, please indicate Make/Model bidding:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + Contractor shall provide 25 Liftmaster, two button visor remotes (892LT-model), or equal.
	+ If not bidding as specified, please indicate Make/Model bidding:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Other Information:**

* + A job site visit is mandatory; vendor will have to inspect and take measurements as there are no plans of the gates available for submission by the agency.
	+ Contractor shall be responsible for disposal of all job related materials, including the existing gates, materials and attachments. A job site roll away dumpster will be able to be placed on site if needed by Contractor. Bids should inclusive of all shipping charges.
	+ Contractor shall supply ALL components and/or hardware needed to complete the installation.
	+ Contractor shall call local utilities before work to be performed before digging anywhere on State of Louisiana’s grounds, to verify the location of utilities, 1-800-272-3020. Repair of any broken lines will be the responsibility of the Contractor.