**Scope of Work:**

Contractor shall furnish all labor, materials, tools, equipment, and supplies necessary to asphalt a new parking area for the Louisiana Department of Corrections, Allen Correctional Center. The parking area will be on Allen Correctional Center property west of the front entry gate and south of Lauderdale Woodyard Road.

**Location:**

Allen Correctional Center

3751 Lauderdale Woodyard Road

Kinder, LA 70648

**Specifications:**

**Contractor shall:**

1. Provide soil test at parking to ensure proper base materials and adhesion of soil cement for laying of asphalt parking lot and entry roads.
2. Provide all equipment and materials required for proper elevations and grading to ensure drainage, and that there will be no “ponding” of water on the parking area or entry roads.
3. Incorporate 8 ½” of soil cement base to the parking area and each of the entry roads.
4. Overlay the soil cement base with 2” of PG 67-22 hot mix asphalt or equal.

**Specify asphalt mix bidding:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

1. All transitions to existing roadways and driveways shall be a smooth and even transition.

**Parking Area:**

Contractor shall pave a 25,410 ft2 visiting center parking area with an approximately 87’ by 29’7” entry road from Lauderdale Woodyard Road and an approximately 270’ by 15’ entry road from the prison front gate. The parking area to be located on existing 2’ raised soil pad. Total paved area including parking area and road is 34,840 ft2.

**Terms and Conditions:**

* An overhead drawing showing the new parking area location is available from the facility upon request.
* There is no demolition of any paving areas or structures required.
* The contractor shall contact Allen Correctional Center Maintenance Manager Christopher Saucier for scheduling of work before starting work
* All work being performed is required during normal business hours Monday through Friday 7:30 A.M. to 4:30 P.M.
* All asphalt to be installed per MFG specifications.
* All work shall meet National Asphalt Pavement Association industry standards and practices.
* Work to be performed according to industry standard, and meet all federal, state and local codes.
* All asphalt to be PG 67-22 or approved equal.
* Parking lot striping or speed bumps are not required.
* Waste materials may be stored adjacent to the construction area until completion of work.
* Upon completion of work all waste materials shall be removed and disposed of by the contractor.
* Contractor employees working on prison grounds are subject to passing a background check.
* Contractor vehicles and equipment are subject to searches.
* Contractor must follow all policy and procedures while performing work on facility grounds.
* No work is required inside the secure perimeter fence of the facility.