**Scope of Work:**

Contractor shall provide all labor and materials in order construct a 40’ x 25’ metal canopy for the Louisiana Department of Military Affairs. Canopy shall be placed in residential area of 6th St. Contractor shall provide all power and water required for construction.

**Location:**

LANG Training Center,

6th St.

Pineville, LA 71360

**Secifications:**

1. Foundation of canopy shall be constructed by contractor using 12” diameter Sono-Tube with 3000 psi concrete. Sono-Tube shall be set at least 24” below surface of soil. All six piers shall have the same elevation of finished concrete in Sono-Tube. Refer to Attachment D - Drawing for details of layout and dimensions of foundation.
2. Structure of canopy shall be metal, refer to Attachment D - Drawing for details of location and dimensions of structure. Columns shall be placed in concrete a minimum of 18” below concrete surface by contractor. Truss to Column of Structure shall be welded. Three trusses shall be used for the structure. Purlin to Truss connection can be welded or fastened with screws: Structure component details are as follows:
   1. Columns – 4” x 4” x 11 Gauge Red Iron
   2. Truss – 4” x 8” I Beam with 3/16” Flange Thickness
   3. Purlin – 2” x 6” x 14 Gauge Red Iron
   4. Roofing – 26 Gauge Burnished Slate Colored R-Panel Sheathing
3. Contractor shall paint the entire iron structure before installing R-Panel Sheathing. Two coats of oil based exterior satin paint shall be applied to all surfaces by the contractor. Color shall be Burnished Slate Roofing color.
4. Roofing shall be installed following manufacturers specifications. Ridge trim matching color of roofing shall be installed along length of structure. Rake trim matching color of roofing shall be installed on both gables of structure by contractor.
5. Contractor shall be responsible for removal of excess material and debris from job site. Contractor shall be required to place construction netting around work site due to location being in residential area. There will be no dumpster available on site for debris removal. Contractor shall be responsible for this requirement.
6. A completed version of the canopy is located in the Parade Field of the site. Contractor can refer to this canopy for structural components and means of installation.

***Project shall be completed no later than 60 days after the issuance of the notice to proceed.***

**General Notes:**

Contractor shall be required to request access to Louisiana National Guard Training Center Pineville. Contractor and all sub-contractors must apply for access badge at the Visitor Control Center BLDG 1460 at Gate 5 of the installation. Visitors shall be required to pass a background check in order to be allowed access to the site. Visitor Control Center is open Tuesday to Friday 6:00 a.m.– 4:30 p.m. Access shall not be granted to conduct site visits Saturday to Monday. Access to the Visitor Control Center is located off Highway 116, not the main gate of the installation behind Wal-Mart. Visitor Control Center personnel can be reached at 318-290-5635.

Facility Engineers operates Tuesday to Friday 7:00 a.m. to 5:30 p.m. Facility Engineers is closed on Weekends and Mondays. Access to personnel and project site must be coordinated during the standard work week. Primary contact method should be email with alternate being phone.

A preconstruction meeting shall be scheduled prior to start of project. A materials/equipment storage area (if required) will be designated by the Project Manager during the course of the preconstruction meeting.

Contractor shall be required to request and execute Louisiana One Call before breaking ground on project site. Copy of clear ticket shall be emailed to Project Manager and kept on file.

All work performed shall meet, or exceed OSHA, parish, state & local codes. All work shall comply with Louisiana Military Department (LMD) safety and environmental requirements. Contractor shall ensure work area is clearly marked with safety barriers, flagging, and signage around the work site as required.

No changes to the project will be allowed, nor will the contractor be paid for any additional work unless an approved Change Order is formally requested and approved in advance.

Contractor shall conduct daily site clean up to ensure a clear work area as well as follow all safety guidelines. All debris and excess material shall be disposed of by the contractor off of the project site and off of Louisiana National Guard Training Center Pineville properly. Contractor shall obtain authorization for placement of contractor provided dumpster with the project manager if needed.

**Project Manager:**

Name: CW3 Michael Hanks

Address: Bldg., 636 I St.

Pineville, LA 71360

Phone: (O) 318-290-5930

Email: [Michael.W.Hanks10.mil@army.mil](mailto:Michael.W.Hanks10.mil@army.mil)