**Scope of Work**:

Contractor shall provide all labor and materials in order to replace 6 exterior light poles with 25’ poles and replace 1 pole with a 15’ pole. Contractor shall provide 2 fixtures per pole for a total of 14 fixtures. Contractor shall remove 1 existing pole (no replacement). Contractor shall remove and replace and replace lace a total of 13 wall pack fixtures as well as 2 flood lights. Contractor shall replace 5 recessed porch lights and replace 5 canopy fixtures.

**General Notes:**

Contractor shall dispose of all debris/trash off site, including but not limited to, all replaced poles and removed poles. Contractor shall coordinate with one of the onsite contacts. Work hours shall take place from 7:30am to 4:30pm CST Monday through Friday, excluding holidays.

**Location:**

Louisiana State Police Region 3 Headquarters

5903 Coliseum Blvd

Alexandria, La 71303

**Site Contacts:**

Lt. Rodney Owens

318-528-9752

[Rodney.Owens@la.gov](mailto:Rodney.Owens@la.gov)

Sherry Jameson

318-715-5439

[Sherry.Jameson@la.gov](mailto:Sherry.Jameson@la.gov)

-Contractor shall remove and replace 7 existing steel poles with 6 Valmont DS330 25’ and 1 Valmont DS330 15’ fatigue resistant soft non-tapered 5” square steel posts, 11 gauge thickness, finished painted bronze with full base cover and appropriate anchoring materials:

**3 - Valmont DS330-500Q250-D5-FP CB-FBC-LAB** (D5mounting 2 drillings @ 180° & 170°) or equal

**Specify Brand/Model/Color of pole bidding:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**2 - Valmont DS330-500Q250-D2-FP CB-FBC-LAB** (D2mounting 2 drillings @ 90° & 270°) or equal

**Specify Brand/Model/Color of pole bidding:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**1 - Valmont DS330-500Q250-D1-FP CB-FBC-LAB** (D1mounting 1 drilling @ 270°)

or equal

**Specify Brand/Model/Color of pole bidding:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**1 - Valmont DS330-500Q150-D5-FP CB-FBC-LAB** (D5mounting 2 drillings @ 180° & 170°) or equal

**Specify Brand/Model/Color of pole bidding:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

-Contractor shall install 2 Keystone 140W, selectable color 3000/4000/5000K LED pole mount light fixtures and pole mounts, bronze in color, per pole:

**14 - Keystone KT-ALED140PS-M2-OSA-NM-8CSB-VDIM** (fixture), or equal

**Specify Brand/Model of light fixture bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**14 - Keystone KT-ALED-PMA-1-KIT** (pole mount), or equal

**Specify Brand/Model of pole mount bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

-Contractor shall remove 1 existing pole (no replacement at this location).

##### -Contractor shall remove and replace 10 wall pack light fixtures with Keystone 50-70 Watt MH Replacement, color select 3K / 4K / 5K, 120-277 Volt, dusk to dawn, bronze in color.

**10 - Keystone KT-WPLED20-S1-8CSB-VDIM,** or equal

**Specify Brand/Model of Wall Pack Light Fixture Bidding:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

# -Contractor shall add 2 Keystone wall pack light fixtures near the southeast corner of the main building and add 1 Keystone wall pack light fixture near the northeast corner of the garage/maintenance building, full cutoff LED wall pack, 120-277V, 60W, 5000K, bronze in color.

**3 - Keystone KT-WPLED60-M2-850-VDIM**, or equal

**Specify Brand/Model of Wall Pack Light Fixture Bidding:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

# -Contractor shall remove and replace 2 flood lights with Keystone 15 watt XFIT LED flood light, knuckle and trunnion mount, photocell, 3K / 4K/ 5K, 2,175 lumens, 120-277V, bronze in color.

**2 - Keystone KT-FLED15-R1A-UNV-8CSB-VDIM**, or equal

**Specify Brand/Model of Flood Light Bidding:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

-Contractor shall remove and replace 5 recessed porch lights with LEDvance 6” round slim downlights, 13 watt, 1200 lumens, 5 color selectable, white in color.

**5 – Sylvania LEDMD6R2A1200ST9SC3**, or equal

**Specify Brand/Model of Porch Light Bidding:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

## -Contractor shall remove and replace 5 canopy fixtures with LED vance 10" canopy fixture, 55W, 6300L, 5000K, 120-277V, bronze in color

**5 – Sylvania CANOPY3A/055UNV750/10S5/BZ**, or equal

**Specify Brand/Model of Canopy Fixture Bidding:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**