**DPS State Police Crime Lab**

**376 E. Airport Avenue**

**Baton Rouge, LA 70806**

Description: Mobile Shooting Range

Dimensions: 8ft. W x 40ft. L x 8ft. 6in. H minimum

\*Concrete pads are to be provided by DPS while all other machinery and site work for the installation is the vendor’s responsibility.

\*DPS will provide electrical connection.

\*\*Ensure that the structure/container is constructed/supported in a manner so that it can be relocated from its original placement. The installed contents should be supported so that they are not disturbed, dislocated, or broken from an installation defect.

Color: Grey
Container to include the following:

* Supports most common pistol calibers up to .44 MAG & Rifle rated up to 308 Winchester (7.62 x 51 2800FPS)
* Push button lock to provide secure access to range
* Down range LED lighting
* Shelving for shooters
* A sloped bullet trap
* 360 degree Armor plating
* Engineered MRT HEPA recirculating air filtration with AC and Heat
* Insulation
	+ 2” sound foam on ceiling and walls firing line to bullet trap
	+ 1” drywall and insulation on every wall and ceiling panel
* 1” Rubber Wall Treatments, Firing Line Forward (excludes 2” sound foam on walls)
* Through wall 1inch water connection with shut off valve
* 4’ wide walk through door on main entry
* Sealed rubber floor mats to be installed, caulked and sealed
* Single phase 50amp, 208/220 Power OR 3 phase power
* One (1) year full parts warranty
* Five (5) year structural warranty
* Consumables: minimum 6 pre filters 4 bag filters and 2 HEPA filters
* Onsite training to be provided at customers location during delivery
	+ 1 to 10 DPS agents in Target Trap System cleaning, Safety & HVAC