**Road Overlay- Sallyport 5 to Tower 9**

**Scope of Work:**

The Contractor shall furnish all labor, materials, tools and equipment necessary to pour a 2” compressed asphalt overlay on the road from Sallyport 5 to Tower 9 road leading to the front of the Maintenance Shop for the Louisiana Department of Corrections (DOC).

**Location:**

Dixon Correctional Institute

5568 Highway 68

Jackson, LA 70748

**Area:**

From Sallyport 5 to Tower 9 in front of the Maintenance Shop.

**Specifications:**

* The Contractor shall overlay the road with a 2” compacted thickness asphalt.
* Low places and/or potholes shall be cleaned, tacked and leveled with asphalt by the Contractor.
* The Contract shall mill any low spots or failures in road prior to asphalt overlay.
* The Contractor shall remove all dirt, loose rocks, and other loose debris. No areas shall be overlaid until roadbed is filled, compacted and free of debris.
* The Contractor shall apply a tack coating (liquid tar) SS18H or equal, to entire area before overlay is applied.
* All transitions shall be milled where joined to existing roadways and driveways to maintain a 2” compacted thickness with a smooth and even transition.
* Areas shall be dry and clean before tack and asphalt is applied.
* Finished asphalt surface shall be smooth-surfaced with no voids, rough, or un-compacted surfaces. All finished road surfaces that are not smooth-surfaces shall be removed and replaced with new asphalt by the Contractor.
* Roads shall not hold water after work has concluded.
* All work shall meet National Asphalt Pavement Association industry standards and practices.

**Planning and Scheduling:**

* The Contractor shall contact Maintenance Manager William Bunch 225-634-6101 for scheduling of work before starting work.
* Work hours to be 7:00am to 4:00 pm Monday through Friday unless approved by Maintenance Manager.