**Scope of Work:**

The Contractor shall provide all labor and materials in order to supply and install a warehouse racking system for Louisiana Department of Health (LDH).

**Location:**

Louisiana Department of Health

Office of Public Health

Bureau of Community Preparedness (BCP) Warehouse

2808 Court Street

Port Allen, LA 70767

**Specifications:**

The contractor shall build and install three back-to-back row warehouse racks at the BCP Warehouse location.

The rack shall contain at least 72 bays (containing six pallets per bay).

The racking shall contain three levels (including floor level). There shall be at least 432 pallet positions.

The pallet racking shall be constructed with steel material. The steel uprights shall be 14-gauge with a 3” x 3” closed tube design. The upright dimensions shall be at least 60”D x 12’H with a capacity of at least 20,000 pounds. The beams shall be at least 8 feet in length with a heavy-duty capacity and built with 16-guage steel. The wire decking shall have a capacity rating of at least 2500 pounds. Each bay shall be at least 96”W x 60”D x 144”H. The wire decking shall be at least 5-6 gauge with a 2.5” x 4” mesh pattern with 5 step channels. Anchor bolts shall be Zinc plated grade 2 steel for dry indoor use. Beams, uprights and deck wiring shall be powder coated.

The three back-to-back row warehouse racks shall be placed to correspond with the current warehouse Zone Map.

Any damages to existing property from the Contractor’s activities shall be restored to pre-work conditions by the Contractor at no additional cost to the Louisiana Department of Health, Office of Public Health, Bureau of Community Preparedness.

**General Notes/Terms:**

The Contractor shall dispose of all trash.

The Contractor shall coordinate with the warehouse manager.

Work hours shall take place from 7:30 to 4:00 Monday through Friday.