**Scope of Work:**

The Contractor shall provide all labor and materials in order to install a 1000 gallon above ground propane tank for the Department of Public Safety (DPS).

**Location:**

FETA Pine Country

214 Dutch Harbor Road

Minden, La 71055

**Specifications:**

This new tank shall be tied into DPS’s current system above ground by the Contractor with no digging or trenching required. The new tank shall be placed on a pre-existing concrete pad by the Contractor that is 20 feet wide x 40 feet long x 4 inches high. The cradles shall be approximately 3 feet at the base and approximately 2 feet high. All work shall be pressure tested for leaks by the Contractor.

1000 gallon Propane Tank shall have the following components:

* Two Leg Stands made from 6 inch channel iron
* 100ft 1/8 inch Air Hose
* 1 ¼ inch Internal Valve with flat handle
* Jomar Ball Valve 1 ¼ inch (R250 1 ¼ inch) or equal

**Specify Ball Valve Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

* Two 2”x20’ Schedule 40 DWV PE PVC PIPE
* Rotary Actuator A3213RA or equal
* Adjustable 3-35 PSI High Pressure bottle Regulator
* Rubber Hose 15’ ¼ 3/8 Female Flared Ends
* Pigtail Rubber POL x ¼ IF x 48”
* QCC Quick Fill Coupling x ¼ MPT
* Hydrostatic Relief Valve ME449H or equal

**Specify Relief Valve Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

* Liquid transfer valve ¾ x ¾ with MEH225 or equal

**Specify Transfer Valve Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**General Terms and Conditions:**

* All work shall be performed between the hours of 8 a.m. to 4 p.m. Monday- Friday.
* The Contractor shall clean up all trash and supplies used around the site.