**Scope of Work:**

The Contractor shall furnish all labor, materials, tools and equipment necessary to pour a 2” compressed asphalt over stone patched area of the parking lot of the Joint Emergency Services Training Center (JESTC) Building for the Louisiana Department of Public Safety (DPS).

**Location:**

JESTC

1400 W Irene Road

Zachery, LA 70791

**Site Visit Contact:**

Richard Perry

225-978-8287

**Specifications:**

* All work shall meet National Asphalt Pavement Association industry standards and practices.
* Finished asphalt surfaces shall be smooth-surfaced with no voids, rough or un-compacted surfaces. Any finished asphalt surface that is not smooth-surfaced shall be removed and replaced with new asphalt by the Contractor.
* The Contractor shall remove all dirt, loose rocks and other loose debris before overlaying.
* Areas shall be dry and clean before tack and asphalt is applied by the Contractor.
* All transitions shall be milled where joined to existing roadways and driveways to maintain a 2” compacted thickness with a smooth and even transition by the Contractor.
* The five red areas (125 square yards) on the attachment shall be dug out, cleaned, tacked and leveled with 6” of asphalt by the Contractor.
* The green area (3,175 square yards) on the attachment shall be milled 2", a tack coating (liquid tar) SS18H or equivalent applied and then overlaid with 2” compacted thickness asphalt by the Contractor.

**Specify Coating Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

* The dark blue area (120 square yards) on the attachment shall be dug out, cleaned, tacked and leveled with 10" of asphalt by the Contractor.

**Planning and Scheduling:**

* The Contractor shall also include mobilization and demobilization costs.
* The Contractor shall be responsible for removal of any and all waste material generated by this project.

****