**Scope of Work:**

The Contractor shall provide all labor, materials, tools, and equipment necessary to construct a metal building to park campers underneath for Louisiana Department of Corrections (DOC).

**Location:**

Rayburn Correctional Center

27268 Hwy 21 North

Angie, Louisiana 70426

**Site Visit Contacts**

Hugh Magee 985-661-6414

Adam Wilson 985-661-6413

**Specifications:**

* 30’W x 120’L x 13.5H Steel framed columns & roof system on concrete footings
* Steel columns and rafters
* 26 gauge Galvalume roof panels with galv. Metal trims & required fasteners. {screws, bolts, anchor bolts}

Stamped engineered plans:

* Foundation Spot Footing plans included
* 5 psf. ground snow load
* 135 Mph. wind speed, exposure ‘C’
* Building code: 2021 IBC

Building and site requirements:

* Roof snow load; 4 psf.
* Soil bearing capacity: 1500 psf.
* Building risk category: II

Building dimensions:

* Width- 30’-0”
* Length: 120”-0”
* Eave height: 14’
* Roof pitch: 4:12
* Quantity of Sidewall bays: 6
* Quantity of End-wall bays: 1

Sheeting & Trim:

* Roof type: PBR panel 26 gauge GLAMPLUS
* Roof color: Galvalume plus
* Eave trim: Galvalume plus

**General Notes/Terms:**

* The Contractor shall be responsible for delivery and pickup of material/ supplies needed to complete project.
* The lay down site will be provided by Rayburn Correction.
* Disposal of all materials, and debris shall be the responsibility of the Contractor.
* Engineered drawings and engineered spot foundation plans to be provided.
* The Contractor shall coordinate all work with the Agency.

