**Scope of Work:**

The Contractor shall furnish all labor, materials, tools and equipment necessary to pour a 2” compressed asphalt overlay at two locations for the Louisiana Department of Corrections (DOC).

**Site Visit Contact:**

William Bunch

225-634-6101

**Location #1:**

Dixon Correctional Institute

5568 Highway 68

Jackson, LA 70748

**Specifications:**

* The Contractor shall overlay the parking lot with a 2” compacted thickness asphalt, including 4” (Hot Mix Asphalt) compacted thickness patches for failure spots.
* Low places and/or potholes shall be cleaned, tacked and leveled with asphalt by the Contractor.

* The Contractor shall mill any low spots or failures in parking lot prior to asphalt overlay.
* The Contractor shall remove all dirt, loose rocks, and other loose debris. No areas shall be overlaid until roadbed is filled, compacted and free of debris.
* The Contractor shall apply a tack coating (liquid tar) SS1H or equal, to entire area before overlay is applied.

**Specify Tack Coating Bidding**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* All transitions shall be milled where joined to existing roadways and driveways to maintain a 2” compacted thickness with a smooth and even transition by the Contractor.

* Areas shall be dry and clean before tack and asphalt is applied by the Contractor.
* Finished asphalt surface shall be smooth-surfaced with no voids, rough, or un-compacted surfaces. All finished surfaces that are not smooth-surfaces shall be removed and replaced with new asphalt by the Contractor.
* Roads/parking lot shall not hold water after work has concluded.
* All work shall meet National Asphalt Pavement Association industry standards and practices.

**Location #2:**

Compound Four

2500 Creekfield Rd.

Jackson, LA 70748

**Specifications:**

* The Contractor shall overlay the parking lot with a 2” compacted thickness asphalt.
* Low places and/or potholes shall be cleaned, tacked and leveled with asphalt by the Contractor.
* The Contract shall mill any low spots or failures in the road prior to asphalt overlay.
* The Contractor shall remove all dirt, loose rocks, and other loose debris. No areas shall be overlaid until roadbed is filled, compacted and free of debris.
* The Contractor shall apply a tack coating (liquid tar) SS1H or equal, to entire area before overlay is applied.

**Specify Tack Coating Bidding**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* All transitions shall be milled where joined to existing roadways and driveways to maintain a 2” compacted thickness with a smooth and even transition by the Contractor.
* Areas shall be dry and clean before tack and asphalt is applied by the Contractor.
* Finished asphalt surface shall be smooth-surfaced with no voids, rough, or un-compacted surfaces. All finished surfaces that are not smooth-surfaces shall be removed and replaced with new asphalt by the Contractor.

* Roads shall not hold water after work has concluded.
* All work shall meet National Asphalt Pavement Association industry standards and practices.

**General Terms and Conditions:**

* The Contractor shall contact Maintenance Manager William Bunch for scheduling of work before starting work.
* Work hours to be 7:00am to 4:00 pm Monday through Friday unless approved by Maintenance Manager.