**Aerator Specs**

**Aerator Unit:**

* Tractor Mounted with rear 3-point hitch connection, PTO operated with 540 or 1000 Connected
* Minimum working width of 63 inches - Maximum working width of 83 inches
* Solid and Hollow tine options
* Adjustable working depth up to 10.5 inches
* Hole spacing per RPM minimum 2.5 inches - 7.5 inches
* Jolt and Vibration damping system (minimizes jolts and vibrations due to hitting unknown obstacles unground)

**Overall dimensions:**

* Minimum length 47 inches - Maximum length 55 inches
* Minimum width 66 inches - Maximum width 104 inches
* Minimum height 47 inches - Maximum height 48 inches

**Must Include Options**:

* *Turf Hold Down Kit 12mm*
* *Turf Hold Down Kit 24mm*
* *Windrow Kit*

*\*All parts required for installation of above items as a single kit included*

* *Hydraulic Front Roller Depth Adj. Kit*

*\*Must be Pre-installed*