**\*\*If bidding other than specified, please provide manufacturer’s specs for “or equal” items. \*\***

**Scope of work:**

The Contractor shall furnish all labor, materials, equipment and tools to install a Gate Control Panel on Sallyport 5 and install a remote door control system for the Infirmary Door for the Louisiana Department of Corrections (DOC).

**Site Visit Contact:**

Will Bunch

225-634-6101

**Location:**

Dixon Correctional Institute

5568 Highway 68

Jackson, LA 70748

**Scope of Work:**

* The Contractor shall add two swinging gates, interlocked.
* The Contractor shall provide one new face plate with updated graphics.
  + Graphic Control Panel Faceplate components consist of Allen Bradley pushbuttons, switches and contact blocks along with low voltage L.E.D.s and all associated wiring and cables or Equivalent

**Specify Brand/Model Bidding**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* Service shall include installation of two FA gate locks.
* The Contractor shall provide technicians on-site to install the remote door control system with two keypads and one 9500 Retro Fit lock with surface mount lock tube.
* The Contractor shall provide electrical terminations to the new equipment.
* The Contractor shall re-use existing wire and cable as much as possible.
* The Contractor shall re-use existing power.
* The Contractor shall provide installation and termination of the remote door control system.
* The Contractor shall provide offsite system engineering and programming.
* The Contractor shall provide onsite start-up, testing and commissioning of the system.
* The Contractor shall provide training to owner on system.
* The Contractor shall provide a 1-year warranty on parts and labor.

**System shall include a minimum of:**

* MAC-RDC (Remote Door Controller) or Equivalent - Quantity: 1

**Specify Brand/Model Bidding**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* ENC-4R (18” x 18” x 4.5” Enc for MAC-4R(x) - Quantity: 1

**Specify Brand/Model Bidding**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* PWR-24V-100W (Phoenix 24VDS, 100 Watt Power Supply) or equal- Quantity: 1

**Specify Brand/Model Bidding**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* LT-IP (Lon-Talk to Ethernet Adapter) or equal - Quantity: 1

**Specify Brand/Model Bidding**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* IP-8PORT-POE (Trendnet TEG-S82g Switch) or equal - Quantity: 1

**Specify Brand/Model Bidding**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* HP-Pro-Mini-G9 (HP-Pro-Mini 400 G9 i7 16GB Desktop) or equal - Quantity: 1

**Specify Brand/Model Bidding**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* VZ-22-MHD (Viewsonics 22” Monitor w/Spr – Black) or equal - Quantity: 1

**Specify Brand/Model Bidding**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* HID-40KNKS-00-0000 (Signo 40K, Reader Keypad unit) or equal - Quantity: 2

**Specify Brand/Model Bidding**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* Airtaq (9500 Retro Fit Lock with 36” lock tube) or equal - Quantity: 1

**Specify Brand/Model Bidding**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* Wind City Wire (20’ Conduit and Wire) or equal- Quantity: 1

**Specify Brand/Model Bidding**: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**General Terms:**

* The Contractor shall be responsible for delivery and pickup of materials/supplies needed to complete project.
* The project shall include a startup performance check. The system must be complete and fully operational.
* Disposal of all materials, and debris shall be the responsibility of the Contractor.
* The Contractor shall be responsible for any damages caused during this project.
* Work to be performed according to industry standard, and meet all federal, state and local codes.
* The Contractor employees are subject to passing a background check.
* The Contractor vehicles and equipment are subject to searches.
* The Contractor must follow all policy and procedures while performing work on facility grounds.
* All work shall be performed during normal business hours: 7:00 AM – 3:00 PM Monday – Friday.