Specifications must meet or exceed all requirements listed below.

Wheelbase 200 FT.

Engine and Equipment

Engine: Detroit DD 13 - 485 HP w/Intebrake or equal.

Air Compressor: Naturally Aspirated

Air Cleaner: Standard   
Fan Hub: 2 Speed

Radiator Cooling Module: 1,240 Square Inches Minimum

Radiator Bug Screen: Mounted Between Hood and Grille

Exhaust: Mounted Under Cab between Frame with Tail Pipe (No Stacks)

Fuel Filter: Standard Fuel/Water Separator   
Alternator: 160 AMP Minimum, Brush Type

Batteries: 3 GP31 Threaded Post with Battery Disconnect Switch or Equal

Starter: 12-Volt System

Transmission

Transmission: 10 Speed Manual

Front Axles & Equipment

Front Brakes: Disc Brakes

Splined Rotors: Front Air Disc Brakes with Aluminum Hubs

Front Hubs: Aluminum Hub Pilot

Hub Caps: Front Vented

Slack Adjusters: Automatic

Front Springs Taperleaf 12,000 LBS. with Shocks

Rear Axles & Equipment

Rear Axles Ratio: 323

Rear Brakes: Disc Brakes

Driver Controlled Differential Lock Rear Axles

Air Suspension Dump Valve

Rear Springs 40,000 LBS. with Shocks

Air Ride Rear Suspension with Single Leveling Valve

Tires & Wheels

Front Tires: 295/75 22.5 Low Profiles

Rear Tires: 295/75 22.5 Low Profiles (None Grips)

Front Wheels: Alcoa Al Utra One Wheel

Rear Wheels: Alcoa Al Utra One Wheel

Or Tires and Wheels Rated by Manufacturer

Frame & Equipment

Bumper: Stainless Steel (Tapered) with LED HD Fog Lights   
Front Tow Hooks (2)

Storage Box with Polished Aluminum Cover RH Side In Front of Half Fender

Aluminum Grated Deck Plate on Frame between Cab and 5th Wheel   
Stainless Steel (2) Half Fender Covers

Parallel Style Polished Aluminum Battery Box Module with Integral Step for Cab and

Passenger

Polished Aluminum Steps Driver & Passenger

Fifth Wheel Release: Left Hand Driver's Side

Fifth Wheel: Air Slide Rail Minimum 3 FT.

Fifth Wheel Height: 48 Inches

Fuel Tanks & Equipment Must Meet or Exceed Below Spec

Tanks: Dual 80 Gallons, Aluminum with Stainless Steel Straps

Def Tank: 15 Gallons Minimum with Stainless Steel Cover

Cab & Equipment

Day Cab with Smart Sound or Equivalent Insulation Package

Air- Ride Cab Dual Air Bags

Full Top Air Fairing with Cab Extenders

Sun Visor Front of Cab

Radio: AM/FM/WB/USB/Bluetooth with (4) Speakers

Hood: Front Mounted Mirrors Drivers & Passenger Side

Cruise Control: Set to Hold Minimum 75 MPH

Instrument Panel: Standard Gauge Package

Driver's Seat: Legacy Silver Air Ride with Dura Leather Color (Gray)

Passenger Seat: Standard High Back Air Ride with Dual Armrest

CB Antennas: Dual Prewired Cab Mounted

Minors: Dual Moto Heated Mirrors, LH & RH Remote Controlled

Windows: Electric Powered with Electric Door Locks

Long Aluminum Grab Handles LH/RH

Utility Lights (2) Mounted on Rear of Cab

Steering Wheel: 18 Inch 4 Spoke

Steering Column: Adjustable Telescoping and Tilt

Gauge: Dual Axles Temp & Transmission Oil

Gauge: Tractor Air Suspension Pressure Gauge

Drivers Information Center: Speedometer, Tachometer, Fuel Gauge, DEF Gauge, Engine

Coolant Temp., Oil Pressure & Oil Temperature, Air Application Gauge , All Warning

Lamps, Engine Hour Meter, Outside Air Temperature Readout, Turbo Charger

Pressure Read-Out

Cab Floor: Black Rubber Floor Mats

Lights *&* Instrument

Headlamps: Dual LED

Marker & Cab Lights (5) LED

Turn Signals Lights: LED

Stop Tail Lights: LED Red & (2) LED Backup Lights Flange Mounted with LED License

Plate

Standard Circuit Breakers

Electrical Audio Backup Alarm

Switches & Wiring: (2) Dash Mounted Extra Factory Wired Auxiliary Switches

Air Equipment

Air Dryer: Bendix or Equal

Air & Electrical Supply Kit: Tractor BOS- Mounted Kit, Cab Mounted Slide Bar, Spring

Hanger

Composite Glad Hand & Light Plug Holder Mounted On Back Of Cab.

Dash Mounted Trailer Air Supply Valve, Trailer Hand-Controlled Valve, and Hoses/Fittings

for Valves,

Dash Mounted Parking Brake Valve and Tractor Protection Valve.

Nylon Air Tubing in Frame & Cab

Air Horn: Single Horn Mounted on Cab

Trailer ABS Electric Supply SAE J560 7 Pin Connectors

Paint Color

Paint: Base Coat/Clear Coat - White

Freightliner CA126DC or Equal