**\*Fax Bid\* Vehicle Equipment - DOC**

Unit Price Shall Be Inclusive Of All Labor, Materials, Equipment, Tools, And Associated Costs To Furnish And Install All Of The Below Items.

All Items Must Be Compatible With 2024 Dodge Durangos.

DOC Will Deliver Vehicles To Vendor Location.

Vendor Must Be Located No Greater Than 130 Miles Away From:

504 Mayflower Street, Bldg 6 3rd Floor

Baton Rouge, LA 70802

**Item 1: Interior Front Light Bar (Feniex QT1915-SD Or Equal)**

* Must Include Blue And White Colors
* LED Count Of 192 Per Unit Minimum
* Programmable Settings: 21 Flash Patterns And CRUISE
* Maximum Current Draw Of 10 Amps
* 60⁰ Optic Spread Minimum
* Must Have Aluminum Housing
* Must Have Polycarbonate Lens
* To Include Mounts
* Qty 1

Specify Brand Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Model Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Colors Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify LED Count Per Unit Bidding: \_\_\_\_\_\_\_\_\_\_\_

Specify Programmable Settings Bidding: \_\_\_\_\_\_\_\_\_

Specify Current Draw Bidding: \_\_\_\_\_\_\_\_

Specify Optic Spread Bidding: \_\_\_\_\_\_\_\_

Specify Bidding Aluminum Housing: Yes \_\_\_\_ No \_\_\_\_\_

Specify Bidding Polycarbonate Lens: Yes \_\_\_\_ No \_\_\_\_\_

Specify Bidding Includes Mounts: Yes \_\_\_\_ No \_\_\_\_\_

Specify QTY Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Item 2: Rear Glass Light Bar (Feniex QT0620-SD Or Equal)**

* Must Include Blue And White Colors
* LED Count Of 27 Per Module Minimum
* LED Count Of 162 Per Unit Minimum
* Programmable Settings: 21 Flash Patterns And CRUISE
* Maximum Current Draw Of 6 Amps
* 60⁰ Optic Spread Minimum
* IP 67 Protection Rating Minimum
* To Include Mounts
* Must Have Aluminum Housing
* Must Have Polycarbonate Lens
* Qty 1

Specify Brand Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Model Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Colors Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify LED Count Per Module Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify LED Count Per Unit Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Programmable Settings Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Current Draw Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Optic Spread Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify IP Protection Rating Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Bidding Aluminum Housing: Yes \_\_\_\_ No \_\_\_\_\_

Specify Bidding Polycarbonate Lens: Yes \_\_\_\_ No \_\_\_\_\_

Specify Bidding Includes Mounts: Yes \_\_\_\_ No \_\_\_\_\_

Specify QTY Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Item 3: Under Mirror Lights (Feniex QQUM-0121 Or Equal)**

* Must Include 3 Mode Technology
* 60⁰ Optic Spread Minimum
* 27 LED Count Minimum
* Programmable Settings: 14 Flash Patterns And CRUISE
* Current Draw 1 Amp Maximum
* IP 67 Protection Minimum
* To Include Mounts
* Qty 2

Specify Brand Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Model Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Bidding 3 Mode Technology: Yes \_\_\_ No \_\_\_

Specify Optic Spread Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify LED Count Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Programmable Settings Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Current Draw Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify IP Protection Rating Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Bidding Includes Mounts: Yes \_\_\_\_ No \_\_\_\_\_

Specify QTY Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Item 4: Grille Lights (Feniex QQMS-8101 Or Equal)**

* 1 Amp Draw Maximum
* Must Include 3 Mode Technology
* 60⁰ Optic Spread Minimum
* Programmable Settings: 14 Flash Patterns And CRUISE
* IP 67 Protection Minimum
* To Include Mounts
* Qty 2

Specify Brand Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Model Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Current Draw Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Bidding 3 Mode Technology: Yes \_\_\_ No \_\_\_

Specify Optic Spread Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Programmable Settings Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify IP Protection Rating Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Bidding Includes Mounts: Yes \_\_\_\_ No \_\_\_\_\_

Specify QTY Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Item 5: Cargo Side Windows (Feniex QQ-0220 Or Equal)**

* 2 Programmable Color Settings Minimum
* Must Include Blue And White Color Setting
* Programmable Settings: 14 Flash Patterns, CRUISE, And Flood
* IP 67 Protection Minimum
* 60 ⁰ Optic Spread
* Field Serviceable and Plug-In Play Connectivity Not Required
* To Include Mounts
* Qty 2

Specify Brand Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Model Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Number Of Programmable Color Settings Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Bidding Blue And White Color Setting: Yes \_\_\_ No \_\_\_

Specify Programmable Settings Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify IP Protection Rating Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Optic Spread Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Bidding Includes Mounts: Yes \_\_\_\_ No \_\_\_\_\_

Specify QTY Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Item 6: Handheld Controller/Siren (Feniex C-5017 Or Equal)**

* 100watts Siren Output Minimum
* 20 Amp Max Current Draw
* 23 Programmable Siren Tones Required
* To Include Mounts
* Qty 1

Specify Brand Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Model Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Siren Output Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Maximum Current Draw Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Number Of Programmable Siren Tones Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Bidding Includes Mounts: Yes \_\_\_\_ No \_\_\_\_\_

Specify QTY Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Item 7: Speaker (Feniex S-2009 Or Equal)**

* Sound Output Range Is Dispersion 80⁰
* Must Have Polycarbonate Housing
* Must Meet SAE J1849 Standards
* To Include Mounts
* Qty 1

Specify Brand Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Model Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Sound Output Dispersion Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Housing Material Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Compliance With SAE J1849 Bidding: Yes \_\_\_ No \_\_\_

Specify Bidding Includes Mounts: Yes \_\_\_\_ No \_\_\_\_\_

Specify QTY Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Item 8: Wiring Kit**

* To Include All Necessary Tools And Supplies For Installation, Including But Not Limited To Switch, Fuses, Wiring, And Wire Loom
* Qty 1

Specify Bidding Inclusion Of All Necessary Tools And Supplies For Installation:

Yes \_\_\_ No\_\_\_

Specify QTY Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Item 9: Transport Cell (Jotto 475-1765 Or Equal)**

* Must Be Constructed With Powder Coated Steel And Polycarbonate
* Qty 1

Specify Brand Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Model Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_

Specify QTY Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Bidding Powder Coated Steel And Polycarbonate Construction: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\*Specify Distance (Miles) From 504 Mayflower Street, Bldg 6 3rd Floor

Baton Rouge, LA 70802\*: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Warranty Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Specify Days To Completion ARO Bidding: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_