**ATTACHMENT B – Revised per Addendum No. 2**

**Dated: 06/10/2025**

**RFx number: 3000024634**

**Contract Title: Harley Davidson Motorcycles – DPS**

**Specifications**

1. **Model Year:**

Motorcycles shall be new, of current manufacture, and production models. Production schedule for model year bid shall be provided with bid. Updates to the production schedule shall be submitted within one week of manufacturer publishing.

1. **Emissions Standards:**

In order to be considered for an award, all vehicles, unless specified herein, must be approved for delivery in the 48 continental United States.

1. **Louisiana Safety Inspection Sticker**

**Do not include the cost of the safety inspection in your bid price.** Applicable Safety Inspection Sticker cost, as determined by LA Dept. of Motor Vehicles (DMV) guidelines, will be added to awarded lines, based on the parish in which the Dealer is domiciled. Two Year new vehicle Safety Inspection Stickers will be required for participating Dealers, in participating parishes. One Year Safety Inspection Stickers will be required for all other vehicles not covered above. Dealers located in Orleans Parish will have the cost of an East Baton Rouge Parish Inspection Sticker added to awarded lines ($18).

Dealership domiciled in \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Parish.

* Dealership authorized to issue LA new vehicle 2 Year Safety Inspection Sticker.
* Dealership authorized to issue LA 1 Year Safety Inspection Sticker
* Dealership is not authorized to issue, but will obtain a 1 Year sticker prior to delivery of vehicles.
1. **Pre-Delivery Servicing and Adjustment**
	1. Dealer shall not attach any Dealer identification advertising or similar material to the motorcycle.
	2. The motorcycle shall be clean and free from defects when delivered.
	3. Prior to acceptance by the State, the Dealer shall service and adjust each motorcycle for operational use, to include as a minimum, the following:
		1. A Louisiana temporary license plate
		2. A Louisiana safety inspection sticker
		3. All motorcycles will be delivered with a fuel gauge digital readout indicating minimum 40 miles to empty.
		4. Focusing of lights
		5. Tuning of engine
		6. Adjustment of accessories
		7. Checking of electrical, braking and suspension systems
		8. Charging of battery
		9. Alignment of front end
		10. Inflation of tires
		11. Balancing of all wheels
		12. Complete lubrication of engine, chassis and operating mechanisms with recommended grades of lubricants for the ambient air temperature at the point of delivery.
		13. All fluids filled to OEM’s recommended capacity
2. **Documents**

Each vehicle shall be delivered with complete certification of origin, odometer disclosure statement, tag application, warranty, owner's manual, copy of Dealer’s inspection and service check sheet and any other necessary credentials. Dealer will supply the Agency with at least one copy (printed or electronic) of technical information, manuals, service manuals, suggested time schedule/flat rate manual, parts list, special parts list and bulletins related to each make and model of vehicle(s) purchased at Dealer’s invoice cost. Dealer must set up notification through OEM to same Agency for receiving new bulletins, vehicle updates, service alerts or recalls.

1. All applicable requirements and standards of the Environmental Protection Agency regulations, Federal Motor Vehicle Safety Standards, Federal Motor Carrier Safety Administration regulations and Tire and Rim Association Inc. that are in effect on the date of manufacture, shall apply. Vehicle(s) furnished to meet indicated specifications, including all equipment and accessories, shall comply with the regulations applicable to current model year vehicle: Title 49, Code of Federal Regulations, Chapter iii, Federal Highway Administration, Department of Transportation and State of Louisiana highway regulatory laws.

All vehicles shall be approved and marketed by the OEM. Full OEM literature, parts, service, technical support and warranties shall be available.

1. **Warranty**

All vehicles procured under these specifications shall be fully warranted against defective materials or workmanship by the OEM program for a period of not less than 36 months or 60,000 miles from date of delivery and acceptance. However, if additional warranty coverage on the whole or any components of the vehicle, in the form of time and/or mileage including any pro rata arrangements, is normally extended to commercial customers, the State shall receive corresponding warranty benefits.

1. **Standard Equipment**
	* 1. All vehicles offered under this solicitation shall be equipped with all OEM equipment advertised as "standard fleet equipment", unless otherwise specified herein, and should be installed through OEM program.
		2. Deletions from "standard equipment" will not be accepted, unless otherwise specified.
		3. In the specifications, where standard equipment is listed, items less than standard equipment will not be accepted, unless otherwise specified.

**Motorcycle Specifications: Harley Davidson Road King (FLHP)**

**Exterior:** Birch White

**Highlights:**

* Mechanical Adjustable Actuation Clutch
* Limited 3 year, 60,000 mile factory warranty
	+ Police Duty use only
	+ Fully Transferable
	+ Expires at 3 years or 60,000 miles, whichever comes first

**Model Unique Features**

* RDRS Rider Safety Enhancements
	+ Cornering Enhance ABS (C-ABS)
	+ Cornering Enhance Electronic Linked Braking (C-ELB)
	+ Cornering Enhance Traction Control System (C-TCS)
	+ Drag-Torque Slip Control System (DSCS)
	+ Vehicle Hold Control (VHC)
	+ Tire Pressure Monitoring System (TPMS)
* Fan-assisted oil cooler
* Floating, dual-front open brake rotors
* 2-1-2 exhaust with dual tapered mufflers
* Dual law enforcement blue license plate marker lamps (OEM standard)
* Pivoting footboards with heel/toe shift lever
* Dual halogen headlight
* Reflex Linked Brembo Brakes with ABS
* 4-piston front and rear caliper
* Trigger switch activation allows approx. 15 minutes of power to police emergency equipment with ignition off
* Independent hazard warning switch
* Emergency light switch with four functions and individual indicator lights for: Off, Both Front and Rear On, Front On only, Rear On only
* Saddlebags with One-Touch latch, standard saddlebag guard and luggage locks, common with ignition key

**Dimensions**

* Length: 96.5 in.
* Overall Width: 37 in.
* Overall Height: 56.3 in.
* Seat Height: Laden 27.3 in. Unladen 31.1 in.
* Ground Clearance: 5.3 in.
* Rake: 26
* Fork Angle: 29.25
* Trail: 6.7 in.
* Fuel Capacity: 6 gallon (warning light at approximately 1 galllon)
* Weight:
	+ As Shipped: 805 LB
	+ In Running Order: 842 LB
	+ Gross Vehicle Weight Rating: 1360 LB
	+ Gross Axle Weight Rating
		- Front: 500 LB
		- Rear: 927 LB

**Engine**

* Engine: MDwaukee-Eight 114 Engine
* Valves: Pushrod-operated, overheard valves with hydraulic, self-adjusting lifters; four valves per cylinder
* Bore x Stroke: 4.016 in. x 4.5 in.
* Displacement: 114 cu. in.
* Compression Ratio: 10.5:1

**Performance**

* Engine Torque:
	+ North America: 123 ft. lb @3000 RPM
* Lean Angle:
	+ Right 32"
	+ Left 32"
* Fuel Economy: 43 MPG

**Chassis**

* Frame: Mild steel; tubular frame; two-piece stamped and welded backbone; cast and forged junctions; twin downtubes; bolt-on rear frame with forged fender supports; MIG welded.
* Swingarm: Mild steel, two-piece drawn and welded section, forged junctions, MIG welded
* Front Fork: 49 mm Dual Bending Valve
* Rear Shocks: Premium standard height hand-adjustable rear suspension
* Wheels: Impeller Cast Aluminum
	+ Front: 17in. x 3 in.
	+ Rear: 16in. x 5 in.
* Brakes:
	+ Caliper Type: 32 mm, 4-piston front and rear
	+ Rotor Type {diameter x width}:
		- Front: (dual floating rotors) 11.8 in x 0.2 in.
		- Rear: (fixed rotor) 11.8 in. x 0.28 in.
	+ Anti-lock Braking System: Standard
* Suspension Travel
	+ Front Wheel: 4.6 in.
	+ Rear Wheel: 3 in.

**Each unit to be fitted with add-ons and to be installed prior to delivery (Unit required to be fitted with specified quantities as listed).**

**Add-Ons:**

|  |  |  |
| --- | --- | --- |
| **PART NUMBER** | **DESCRIPTION** | **QUANTITY** |
| 68000287 | KIT, LTG, LIGHTING ARRAY | 1 |
| 69202610 | KIT, HARN/WRG,PWR INP,POCE | 1 |
| 90201903 | SADDLEBAG GUARD | 1 |
| 68000279 | POWER BOX | 2 |
| 69200308 | SOCKET, TERMINAL | 18 |
| 72038-71A | SOCKET, TERMINAL | 1 |
| 72168-07 | SOCKET, TERMINAL | 5 |
| 72414-07BK | HOUSING, 6WAY | 1 |
| 72907-11 | HOUSING, 4 WAY PIN | 1 |
| 72908-11 | HOUSING, 4 WAY SOCKET | 7 |
| 72909-11 | TERMINAL, PIN | 2 |
| 76000853 | AMP | 1 |
| 69200597 | AMP MOUNT | 1 |
| P32F2BB | BLUE PAR32 W/DRIVE LIGHT | 1 |
| TIONHDSS | TION SIDE SADDLE BAG MOUNT | 2 |
| TIONHDRS | TION REAR SADDLBAG MOUNT | 2 |
| IONSV3BC | ION BLUE W/PUDDLE/ALLEY | 2 |
| PSRASXCR | STRIP LED B/T W/AMBER TS | 1 |
| PSE02FCR | STRIP LIGHT DUE FLASH B/W | 1 |
| IONHD2FM | FLHP FORK LED MNT KIT | 2 |
| TLI2E | ION T-SERIES DUO B/W | 8 |
| TLMI2E | ION T-SERIES DUO MINI B/W | 2 |
| M4E | SPLIT COLOR B/W CLEAR LENSE | 4 |
| SA350MB1 | SPEAKER BRACKET | 1 |
| SA350MH | 100 WATT SIREN SPEAKER HD | 1 |
| 65301 | ULTRA BIRGHT LED | 2 |
| 65881R2 | WIG-WAG HARNESS | 1 |
| 67502P-HD | H-D BRUSHED ALUM LIGHT | 1 |
| POLICEBOX or Equal | REAR BOX\*\* | 1 |
| 44340859 or Equal | SEAT RISER\* | 1 |
| 54395-220015 or Equal | RISER BOLT – ¼” 20 Bolts  | 2 |
| AVS-X19-15 | BLACK SPACER 4 PACK | 1 |
| 2120-1164 | HARNESS SMART CNTRL BRK | 1 |
| 2106-0581 | TAKE DOWN SWITCH | 1 |

**\*Seat Riser Specifications:**

* Riser heights will vary from approximately 1.5” to 2.5” and made of strong ASA Plastic with threads for ¼” 20 bolts. Height to be determined at the time of order.

**\*\*Police Box Specifications:**

* Police box to be made entirely of .125 gauge, 5052 Aluminum with a spray-in liner.
* Box Dimensions: 21 ¼ ” L x 15 ¼” W x 7” H
* Lid Dimension: 21 ½ ” L x 15 ½ ” W
* Gas Struts: 10” Extended, 18lbs Force (Brand: Genesis GSS 1726UK or equal)
* Latch: Stainless Steel with mini teardrop key lock (Brand: Buyers Product or equal)

****