**These are the minimum specifications for the vehicle described. Where a brand/model is referenced, an equal will be considered.**

**Forklift Truck w/ Universal Mount**

Cummins L9 350hp @ 1050 Lb. /Ft Cummins Integral Engine Brake w/ Variable Geometry Turbo on/off

Battery Disconnect Switch

Jump Start Posts on Frame

Allison 3000rds Automatic Transmission

Trailer Towing Provision

RH under Step After treatment System W/ B Pillar Mounted Tailpipe

6 Gal DEF Tank

Block Heater W/ Receptacle under LH Door

20000 lb. Front Axle

40000 lb. Rear Axles

Driver Controlled Traction Differential - Both Axles

46000 Airliner Rear Suspension 279” Wheel Base

Double Channel Frame

Chrome Bumper

Removable Front Tow Hooks

90 Gal L/H Fuel Tank

385 Front Tires on Wheels

11r22.5 Rear Tires On Wheels

RH Fender Mounted Mirror

Exterior Sun Visor

Power Windows & Locks

High Back Air Suspension Driver Seat

2 Man Tool Box Passenger Seat

Tilt/Telescope Steering Column

**Body & Equipment**

24’6”X 96” All Steel Platform w/ Stake Pockets and Rub Rails

Universal Mounting Kit

10 Reels on Slide Rail Mounted Curb Side

Folding Platform Step Located @ Front of Platform, D/S

Safety Cones W/ Frame Mounted Holder with Integrated Wheel Chocks

60” Toolbox - Barn Door Style

ICC Bumper Integrated Into the Mounting Kit

10 - 4” Nylon Straps & Winch Bar Holder With Bar

Strobe Light Package - 4 Total

**Forklift**

5500 LBS @ 24” load center

Double stage mast, 144” lift height

31x15.5x15 Tires (3)

Hydrostatic drive

56 HP Kohler diesel Tier Four engine

Back up alarm

48” Lumber Forks

Parking Brake

Strobe light

Load backrest

Nav-Reach Single Side Unload

Remote Lift Lower

Block Heater

**Freightliner M2-106 Plus L9 6x4 with Navigator RT5500 Forklift or equivalent**