RFx No.:3000026481 	 Title: *Site Visit* HVAC Maintenance - SOS
Attachment C 
Replacement Filters 
Filters on all air-handlers (5 each) and rooftop units (3 each) shall be replaced monthly with pleated 40% minimum filters. The larger HEPA filters shall be replaced on an annual basis to be completed no later than June 30 of each year. All after-filters shall also be included. 
Filter List 
	Units
	Frequency 
	Filter Type 
	Size 

	All Air-Handlers 
	MONTHLY 
	Pleated 40% Minimum 
	2” 

	All Rooftop 
	MONTHLY 
	Pleated 40% Minimum 
	2” 

	Split Stm Heat Pump Units 
	MONTHLY 
	Pleated 40% Minimum 
	20 X 20 X 1 



