Attachment B – Specifications
RFx #3000026560
These specifications describe the minimum requirements for one new 2026 Peterbilt 548 6’ x 4’ Dump Truck with 16’ DuraClass Dump Body, or equal. This vehicle shall be furnished complete with all necessary operating accessories, equipment, and manuals. The vehicle shall be new, unused, and of the manufacturer’s latest production model meeting or exceeding the requirements listed herein.
A 2026 Peterbilt 548 6’ x 4’ Dump Truck with 16’ DuraClass Dump Body was used to develop the specifications below and establish equivalency criteria. Equipment of similar style, type, character, quality, features, and purpose conforming to the following detailed requirements/specifications will be considered. For evaluation purposes, bidder's proposing an exception/equivalent option/feature to those specified herein, may be required to provide manufacturer/product information (catalogue sheets, detailed specifications, pictures, etc.). This information will be evaluated against the minimum requirements of this specification. Proposed submittals that are determined not to be equivalent to the established criteria will be rejected.
Specifications must meet or exceed all requirements listed below.
[bookmark: _Hlk227760534][bookmark: _Hlk227590276]2026 Peterbilt 548 6’ x 4’ Dump Truck with 16’ DuraClass Dump Body, or Equal:
[bookmark: _Hlk227590348]General
· Year: 2026 or 2027
· Make: Peterbilt
· Model: 548
· Cab: Regular Cab
· Cab-to-Axle: 141"
· Chassis: Class 
Axles & Suspension
· GVWR: 60,000lbs
· Front Axle: 20,000lbs (PACCAR FX-20)
· Rear Axles: 40,000lbs (Dana Spicer DSP41)
· Axle Configuration: 6’ x 4’
· Rear Suspension: Hendrickson HMX400 (Spring – No Air Ride) or equal
· Wheelbase: 210”
· Cab-to-Axle: 140.5”
Powertrain
· Engine: PACCAR PX-9, or equal 
· 370 HP
· 1,250lb-ft torque
· Transmission: Allison 3000 RDS-P Automatic, or equal
· Rear Ratio: 5.57
· Air Disc Brakes (Front & Rear)
· ABS with Off-Road Mode
Suspension & Frame
· Hendrickson HMX EX 40,000lb rear suspension, or equal 
· Heavy-duty 11 5/8" steel frame rails
· Reinforced crossmembers
· PTO (Power Take Off)  & hydraulic provisions installed
Ox Bodies Body Design
· Stampede elliptical dump body (self-cleaning design) or equal too
· AR450 high-strength steel construction
· Crossmemberless understructure
· Telescopic hoist

Body Dimensions
· Length: ~16 ft.
· Side Height: ~48”–54” range
· Capacity: ~15–16 cubic yards
Material Specs
· Floor: 1/4” AR450 steel
· Sides: 1/4” AR450 steel
· Front: 1/4” AR450 steel
· Tailgate: 3/16” AR450 steel
Key Features
· Air-operated high-lift tailgate
· Formed tailgate with bracing
· Spreader chains
· Diamond top rail
· Cabshield (24” projection) 
· Mountain tarp system
Hydraulics & Controls
· Telescopic hoist (Model 74133)
· Hydraulic pump (auto/rotational)
· PTO installed (Allison compatible)
· OX air control tower
· Air tailgate kit
· Hydraulic reservoir (nested design)

Additional Body Equipment
· Mudflaps (30” OX)
· Gravel shields
· Backup alarm
· Body prop
· Removable rear hinge pin
· Cabshield marker lights
Body Finish
· Color: Black (VM9900)
Cab & Interior
· Air ride heated high back with armrest driver seat
· Passenger seat – high back with armrest
· Tilt/telescope steering
· A/C & heater
· Power windows/locks
· Bluetooth radio + USB

Tires & Wheels
· Front: 425/65R22.5
· Rear: 11R24.5
· Polished aluminum wheels
Fuel System
· 100-gallon aluminum tank
· DEF (Diesel Exhaust Fluid) tank (LH (left hand) side - back of cab)
· Fuel coolerElectrical & Safety
· LED lighting
· Daytime running lights
· Backup alarm
· Fire extinguisher
· Triangle kit
· Battery disconnect
Additional Equipment
· PTO (Parker Chelsea or equal)
· Transmission oil cooler
· 45-Ton Pintle Hitch 
· Mudflaps & chassis guards

Total Weight
· Estimated: 15,687 lbs. for chassis. Final vehicle weight includes all permanently mounted body components and equipment as part of the completed build.
Minimum Warranty
· Truck: 1 Year / Unlimited Miles
· Engine: 2 Years / 250,000 Miles
· Emissions: 5 Years / 100,000 Miles

BIDDER’S EXCEPTIONS
Instructions: Bidders should note all exceptions in the space provided below. List the specification from the previous pages, and the exception to that specification. Responses may be typed or hand-written. Handwritten responses must be legible. If additional space is needed, please print a duplicate of this sheet. “Bidder’s Expectations” page(s) should be returned with the bid submittal.
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