Attachment C – 
Specifications
RFx 3000026581

**If bidding other than specified, please provide manufacturer’s specs for “or equal” items. **

Scope of Work:
The Contractor shall furnish all labor, materials, equipment, tools, supervision, and services necessary to remove and replace approximately 6,000 sq. ft. of roofing for the Department of Health (LDH).

Location:
Pinecrest Supports and Service Center
884 Pinecrest Dr. 
Pineville, LA. 71360

LDH Contact:
[bookmark: _Hlk236908165]Glennen Jones; Glennen.Jones@la.gov 
[bookmark: _Hlk236908188][bookmark: _Hlk236908196]Shannon Todd Aymond; Shannon.Aymond@la.gov; (318) 641-2288

Specification:
The Contractor shall perform the following:
· Remove existing roof membrane and replace any rotted insulation board.
· Install new ½" Structodek HD cover board or equal.


          Specify Cover Board Bidding: _____________________
· New HD board shall taper out to edges with a¼" fall minimum.
· All insulation and cover board shall be adhered with Ultraply bonding adhesive or equal.

Specify Bonding Adhesive Bidding: _____________________
· Install and adhere new thermoplastic polyolefin (TPO) membrane to board with adhesive 
· Install new TPO unsupported flashing and secure with aluminum strip.
· Install any related curb flashings
· Install any related wood blocking around perimeter edge.



Terms and Conditions:

· Work area shall be kept clean and orderly throughout the project by the Contractor.

· All debris, fasteners, and scrap material shall be removed from the site upon completion by the Contractor.
· All materials shall be new, of commercial quality, and installed per manufacturer’s specifications. 
· The Contractor shall be responsible for disposal and storage of all materials being removed or installed throughout the project. 
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