
	Attachment B - Specifications		

RFx No.: 3000026665	Title: Forklifts – LADF

Specifications for Food Distribution Forklifts
 Brand: Yale or Approved Equal
 Model: ERP030VT or Approved Equal 

Model Information: 
* Counterbalanced Sit-Down Electric Rider Lift Truck 3,000 lb. 
* Nominal Capacity @ 24” Load Center 

Construction: 
* Key Switch Start 
* Cooler / Freezer Package – Operating Temperatures -20 ℉ to +120 ℉
 * 36 Volt 

Powertrain Options:
* UL Classification Type “E” 

Battery Compartment: 
* 21.5” Battery Compartment
* Battery Compartment With Auxiliary Counterweight Spacer Platform 
* Battery Removal without Rollers – Lift Out 

Mast:
* 3 Stage Full Free Lift Mast – Class II – 187” (4750mm) Maximum Lift Height – 82” (2080mm) Overall Lowered Height – 59” (1505mm) Free Lift Height without Load Backrest – 236” (5980mm) Overall Extended Height With Load Backrest 
* Mast Tilt – 5° Forward / 5° Back 

Carriages & Attachments: 
* 38.5” (977mm) Wide – Class II – Hook Type Integral Sideshift Carriage 
* 48” (1220mm) High Load Backrest Extension

 Forks:
 * 42” Long x 1.6” Thick x 3.9” Wide (1067mm x 40mm x 100mm) – Class II Hook Type – Standard Taper Forks 

Hydraulics: 
* 3 Function (1 Auxiliary) Hydraulic Control Valve
* Mechanical Lever Hydraulic Controls – Seat Side – With Return To Set Tilt 
          
Hoses: 
* 1 Auxiliary Function Hose Group – 2 Hoses Internally Mounted
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 Wheels & Tires: 
* Drive Tires – 18 x 7-8 – Pneumatic Shaped Solid (PSS) – Standard Compound – Lug Tread
* Steer Tires – 15 x 4.5 x 8 – Pneumatic shaped solid (PSS) – Standard Compound 

Operator Compartment: 
* 81.5” (2070mm) Overhead Guard – Grid Style
* Mirrors – Dual Side View – Mounted On The Left And Right Side Of Overhead Guard 
* Display – High Mount – Mounted In Upper Right Corner Of Overhead Guard 
* Fire Extinguisher – 2.5 lb. Dry Chemical
* Rear Drive Handle With Horn Button

 Directional Control: 
* Seat Side Directional Control 
* On Demand Hydrostatic Power Assist Steering 
* Steering wheel With Spinner Knob 
* Steer Column With Infinitely Adjustable Tilt 

Seat: 
* Non-Suspension Vinyl Seat 
* Seat Belt – Black – No-Cinch With ELR (Emergency Locking Retractor)

 Telemetry: 
* Yale Vision Wireless Monitoring with Cellular connectivity – GSM or Approved Equal
* 7 Year, Level 1 Telematic Communication and Portal Fees – Monitoring

 Lights & Alarms:
* Work Lights – LED Plastic Lens – 2 Front and 1 Rear – Rear Combination  
Lights – LED – 2 Brake / Tail / Back-Up
 * Audible Alarm – Reverse Direction Activated – Self Adjusting 82 – 102 dB(A)
 * Amber Strobe Light – Ignition Activated
 * DC to DC Converter – Primary – For Factory Installed Options – 25 Amps / 300 Watts @ 12 Volts

 Warranty:
 * 12 Months / 2,000 Hours Manufacturer’s Warranty, 36 Months / 6,000 Hours  Manufacturer’s Powertrain Warranty

Literature & Nameplate: 
* English Literature Pack and Labels 
 Battery & Charger Accessories: 
* Battery Charging System – Conventional – Includes Single Battery Connector Under The Hood 
* Lead Acid Battery Power – Truck Configured To Operate On Lead Acid Battery Power. Not   To Be Used With Lithium-Ion 
* Battery Connector – Grey SB® 350 
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Additional Items or Accessories: 
* EZF Watering System 
* Direct Fill Link 
* Battery Smart Water Monitor 

* Battery Charger: 36-volt, 3-Phase 700AH Black Diamond Battery Charger, compatible with 208/240/480 VAC input voltage and capable of charging batteries to a maximum capacity of 700 amp-hours (AH). (Or Approved Equal)

* Battery: 680AH/23.6232KWH Concentric Lead Acid Battery – 5 Rated Service Life – Installed and comes with a 5 - year warranty (Or Approved Equal)

 To Be Delivered To:
 Louisiana Department of Agriculture & Forestry 
 5825 Florida Blvd.
 Baton Rouge, LA 70806
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