
Attachment B – Specifications
RFx #3000026707
35 Foot, 60,000 Pound Pintle Hitch Galvanized Trailer
for
The Louisiana Department of Wildlife and Fisheries
Quantity: One new trailer
The trailer shall be a new, heavy-duty, galvanized pintle hitch trailer with a minimum 60,000-lb load capacity and shall meet or exceed the following specifications:
· Overall Length: Approximately 35'-0" 
· Deck Width: 8'-6" 
· Deck Length: Approximately 29'-0", consisting of approximately 24'-0" flat deck and 5'-0" beavertail 
· Construction: Pierced main-beam construction 
· Main Beams: Minimum W14 x 22 lb. per foot, Grade 50 high-tensile steel 
· Crossmembers: 6" I-beam, approximately 3.9 lb. per foot, spaced on approximately 22" centers 
· Side Rails: C8 x 11.5 lb. per foot, Grade 50 high-tensile steel 
· Ramps: Two approximately 7' x 3' air-assisted ramps 
· Decking: 2" nominal oak decking 
· Headboard: 8" structural channel, full width of trailer 
· Suspension: Multi-point spring suspension with radius-type axles; minimum approximately 9,700-lb suspension capacity per point 
· Axles: Three 25,000-lb capacity axles with oil-bath hubs 
· Brakes: Minimum 12" x 4" electric brakes with automatic brake adjustment and spring parking brakes 
· Tires: 12, 235/75R17.5, Load Range H tires, plus spare tire and carrier 
· Wheels: 8-hole steel wheels with hub-piloted design 
· Jacks: Dual electric/hydraulic landing jacks 
· Hitch: 4-position adjustable pintle-eye hitch; approximately 1-5/8" stock and 3" inside diameter 
· Lighting: Flush-mounted LED lighting in rubber grommets 
· Wiring: Modular wiring harness with 7-way electrical plug 
· Finish: Entire trailer shall be hot-dip galvanized or equivalent corrosion-resistant finish 
· Tool Storage: Lockable tool box/lid 
Trailer shall be designed for a minimum 60,000-lb payload capacity and a minimum 65 MPH highway operating speed.
Delivery: Bidder shall state estimated delivery time from receipt of purchase order.
Warranty: Bidder shall provide manufacturer's standard warranty and warranty terms with bid.
Equivalent Equipment: Equipment meeting or exceeding the specifications listed above will be considered. Bidder shall identify the make, model, and specifications of the equipment being offered.
Delivery: The bidder shall include delivery of the specified trailer to the designated delivery location. Vendors located more than 100 miles from the delivery location shall be responsible for delivering the trailer to the designated location at no additional cost to the purchaser.
Delivery Location: 5476 G.C. Highway, Grand Chenier. LA 70643
Distance Requirement: The 100-mile distance shall be measured from the bidder's place of business to the designated delivery location.

2

