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Scope of Work: 
The Contractor shall supply all labor, equipment, supplies, and materials to complete the construction a new parking lot and paving of an existing gravel access roadway for the Department of Public Safety and Corrections (DPS).

Location: 
Joint Emergency Services Training Center (JESTC)
1400 W. Irene Road,
Zachary, Louisiana 70791

Site Visit Contact:
Richard Perry, Richard.perry@la.gov, (225) 978-8287

Specifications:
The project consists of constructing an approximately 120-foot by 120-foot parking lot and paving approximately 1,040 linear feet of existing gravel access roadway. The completed parking area shall accommodate approximately 40 striped parking spaces and shall be graded to provide drainage.

The Contractor shall be responsible for the following:

Parking Lot Construction:
· Remove existing grass and surface material within the approximately 120-foot by 120-foot parking lot area.

· Prepare and grade the designated parking lot area.

· Furnish and install approximately 8 inches of aggregate base material.

· Compact the aggregate base material.

· Furnish and install approximately 2 to 2.5 inches of asphalt pavement over the prepared aggregate base.

· Stripe the completed parking lot to provide approximately 40 parking spaces.

Access Roadway:
· Prepare the existing gravel access roadway.
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· Pave approximately 1,040 linear feet of the existing access roadway.
· Furnish and install approximately 2 inches of asphalt pavement over the prepared roadway/base.

· Complete the roadway in a manner suitable for its intended vehicular use.

Grading and Drainage:
The parking lot shall be graded to provide drainage.
Any drainage structures or additional drainage improvements required beyond grading shall be considered outside the base scope and shall require prior written authorization from the State.

Excavated Material
Dirt and other material removed during site preparation shall be hauled and placed onsite. This cost shall be included in the Contractor’s bid price.
No offsite hauling shall be performed without prior authorization in accordance with applicable State procurement requirements.

General Terms:
· The Contractor shall coordinate the construction schedule with the designated JESTC representative.

· The Contractor shall provide at least 14 days written notice prior to mobilization.

· The Contractor shall coordinate access to the project site with JESTC personnel.

· The Contractor shall perform all work in a professional and workmanlike manner.

· The Contractor shall maintain the project area in a reasonably orderly condition during construction.

· The Contractor shall notify DPS of unforeseen site conditions that may affect the scope, cost, or schedule before proceeding with work outside the approved scope.
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