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                                              Off Road Spike / Icebreaker


Make/Model: Raiko Ice Breaker T15 or approved equal

Included Features & Options:
· Breaks up ice and compacted snow without damage to pavement
· Pushable model designed to be pushed in front of a working machine equipped with a tilt                cylinder
· Flexible and freely rotating spiked roller sections
· Minimum operating weight: 3,800 lbs.
· Minimum working width: 100 inches
· Recommended minimum working machine weight: 11,023 lbs.
· Must be compatible to a JRB-416 hydraulic coupler

