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                    RFx No. 3000026742            Attachment C            Title – Spike Rollers - DOTD 

                               DOTD Bid Specification No. 350-000B, REV. 9/9/2026
                              Off Road Spike / Icebreaker for Wheel Loader with blade

Make/Model: Raiko Ice Breaker P15 or approved equal

Included Features & Options:
· Breaks up ice and compacted snow without damage to pavement
· Pushable model designed to be pushed in front of a working machine equipped with a tilt cylinder
· Dedicated blade located behind spiked roller sections
· Blade able to raise and lower independently of spiked roller sections
· Blade capable of rotating to discharge ice and snow to either side
· Flexible and freely rotating spiked roller sections
· Minimum operating weight: 3,800 lbs.
· Minimum working width: 100 inches
· Recommended minimum working machine weight: 11,023 lbs.
· Must be compatible to a JRB-416 hydraulic coupler

