Attachment C – Specifications
RFx 3000026791

Scope of Work: 
The Contractor shall supply all labor, equipment, supplies, and materials to complete the demolition of a building structure and construction of four modular buildings for the Department of Public Safety and Corrections (DPS).

Location: 
Building Housing Unit
6868 Nicholson Drive
Baton Rouge, LA 70820

Site Visit Contact:
Chief Ed Branch, ed.branch2@la.gov, 
Office: (225) 925-4911, Cell: (985) 515-5864

Specifications:
The Contractor shall be responsible for the following:

Existing Utilities
· The Contractor shall locate and verify all existing underground and aboveground utilities before beginning demolition or excavation by performing the mandatory jobsite visit. 

· The Contractor shall coordinate disconnection of electrical, water, sanitary sewer, storm drainage, natural gas, communications, fire protection and other utilities serving structures to be demolished.

· Utilities to be abandoned shall be disconnected, capped, plugged, or otherwise terminated in accordance with the requirements of the utility provider and authority having jurisdiction 

· Existing utilities, serving structures or site areas to remain shall be protected and maintained in service. Any unknown or unidentified utility encountered during demolition shall be treated as active until verified otherwise. The Contractor shall immediately notify the owner of any unidentified utility or condition that may affect the work
Building Demolition
· Removing existing structures indicated on the drawings in their entirety, including building components, interior and exterior finishes, roofing, mechanical, electrical, plumbing, site connections, and other associated work unless specifically noted to remain.

· Removing existing fountains, footings, piers, slabs, aprons, and other below-grade structural elements associated with structures being removed, unless specifically indicated to remain.

· Removing existing debris, abandoned equipment, concrete, masonry, metal, wood, and other materials within the demolition area.

· Removing demolition debris from the site and dispose of materials at a legal and approved disposal facility.

· The Contractor shall not burn, bury, or abandon demolition debris on the project site. 

· Demolition shall be performed in a sequence that prevents damage to existing structures, utilities, pavement, landscaping, and other items to remain. 

Site demolition
· Removing existing walks, curbs, pavement, concrete, aprons, site structures, fencing, signage, light poles, site equipment, and other side improvements indicated for removal.

· Protecting existing trees, landscaping, pavement, utilities, drainage structures, and other site features indicated to remain.

· Providing temporary fencing and barricades as required to separate demolition operations from occupied areas and public access.

· Maintain safe, pedestrian and vehicle access throughout the project as required by the Agency.

· The Contractor shall control dust, mud, debris, and other conditions resulting from demolition operations.

· Drainage and erosion control. 

· Maintaining existing drainage patterns during demolition and site preparation unless otherwise indicated

· Protecting existing catch basins, train structures, ditches, culvert, and storm drain systems to remain.

· The Contractor shall not allow any demolition debris, soil, concrete, or other materials to enter existing drainage systems.

Final Site Condition
· Upon completion of demolition, the Contractor shall leave the site clean, safe, stable, and ready for subsequent construction. 

· Removing all demolition debris, temporary facilities, equipment, and unused material from the site. 

· Removing all unsuitable material, organic material, debris and abandoned construction from areas to receive new work. 

· Capping & securing all abandoned utilities as required. 

· Backfilling and compacting all excavations and voids created by demolition as required for the new work. 

· Providing temporary stabilization of disturbed areas until the final site construction commences. 

· The Agency shall accept the site prior to commencement of new construction in the affected area.

Renovation Site Plans
· The modular buildings shall be furnished delivered, set, installed, connected, and completed in accordance with the contract documents, approved modular building manufacturer's drawings, engineers, documents, specifications, and all applicable codes and regulations.

· The modular building manufacturer and installing contractor shall review all contract documents prior to fabrication, delivery, and installation

· All modular building components shall be designed, fabricated, transported, set, anchored, and installed in accordance with the requirements of the approved modular building system. 

· Field verify existing conditions, including grades, foundations, utility locations, access conditions, and dimensions, prior to fabrication or installation


Foundation
· Foundations shall be constructed in accordance with the structural drawings and approved modular building manufacturers’ requirements.

· Foundation dimensions, elevations, anchor locations, bearing conditions, and connection requirements shall be verified prior to delivery of modular building units.
 
· The Contractor shall verify that foundations are complete, cured, and ready to receive modular units prior to scheduling delivery.

Site preparation
· Site preparation shall be completed prior to delivery of modular building units. 

· Providing required site grading, drainage, access roads, crane pads, staging areas, and other site improvements required for delivery and authorization. 

· Site grades shall provide positive drainage away from the modular buildings. 

· Verifying final finished floor elevations prior to setting the modular units. 

· The Contractor shall maintain access for delivery trucks, cranes, rigging equipment, fire department access, and emergency vehicles throughout the installation process. 

· Protecting completed site work, utilities, pavements, landscaping, and existing structures during delivery and installation.

General Terms:
· Demolition shall be performed in a safe and controlled manner. The Contractor shall provide all shoring, bracing, barricades, fencing, dust control, temporary protection, and other measures required to protect persons, existing property, and adjacent construction.

· The Contractor shall be responsible for maintaining the structural stability of all existing structures, site features, and adjacent construction that are to remain.

· Do not remove, cut, damage, or disconnect any existing system or component that is to remain in service. 

· The Contractor shall coordinate demolition operations with the owner, utility providers, and all appropriate authorities having jurisdiction. 

· Utilities shall be located by actual field investigation. Do not rely solely upon existing drawings or utility records. 

· The Contractor shall contact all appropriate utility companies and utilize the appropriate utility locating service before excavation. 
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