Attachment C – Specifications
RFx 30000266866

Scope of Work:
The Contractor shall provide all labor, supervision, equipment, materials, transportation, hauling, disposal, site cleanup, permits if required, and incidentals necessary to complete the demolition and removal work for the Department of Agriculture and Forestry (LDAF).

Locations:
Beaver Fire Tower - (32 0145.80 N, -92 39 16.8W)
Elizabeth Fire Tower - (30 77230 N, -92 86159 W)
Pitkin Fire Tower - (30 96117 N, -92 96319 W)

LDH Contact:
Benji Rhame, (318) 481-7647

Specification:
The Contractor shall perform the following:
Beaver Fire Tower
· 125 feet tall

Elizabeth Fire Tower
· 110 feet tall

Pitkin Fire Tower
· 110 feet tall

There are no prints or other specifications available for the towers. A site visit is recommended to become familiar with the tower.

Removal and demolition of the tower, including cutting up, dismantling, and removing the entire tower structure from the property. 
· The method of demolition is at the Contractor’s discretion; however, all tower parts must remain on the landowner’s property when the tower is dropped.

· Everything at the location of the tower, including the foundation, must be removed and disposed of once the demolition is complete.
· There is no minimum required depth for the foundation.

Excavation and removal of the four pyramid-style foundation blocks at the tower 
location. The tower is not connected to any electrical, communications, security, or other utilities.

Backfilling each excavation to the surrounding natural grade/elevation using suitable fill material. There is not a specific dirt or soil required. There is concrete foundation below grade.
Terms and Conditions:
The Contractor shall verify all site conditions, access routes, utilities, and location-specific requirements before submitting a bid and before beginning work.

The Contractor shall protect existing improvements, roadways, gates, fences, utilities, trees, and surrounding property from avoidable damage.

The Contractor shall conduct demolition activities in a safe manner and in compliance with all applicable federal, state, and local laws, rules, regulations, permits, and safety requirements.

The Contractor shall be responsible for proper disposal of all materials at an approved disposal facility or in accordance with applicable laws and regulations.

The Contractor shall not leave demolished material, foundation material, scrap, trash, or debris on site unless specifically authorized in writing by LDAF.

The Contractor shall bring in excavators, skid steers, cranes, dump trucks, or other heavy equipment needed for the demolition.

Reaching out to Louisiana 811 shall be the responsibility of the awarded Contractor.

The bridges and access roads must be in the same shape as they were when the project began.

Vegetation and shrubs on the natural land near the tower may be trimmed as necessary to provide equipment and personnel access.

The Contractor shall submit a demolition plan, safety plan, or equipment plan before beginning work.
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