**ENGINEERING SERVICES WANTED**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| Applications for Engineering Services for the following projects will be accepted until **2:00 p.m., Monday, December 21, 2015. (Your attention is called to the 2:00 p.m. deadline -- exceptions WILL NOT be made). Applications shall be submitted on Standard Form LE-1, (revised April 2000 edition.) These forms are available at the selection board office and on the Facility Planning & Control website at** [**www.doa.la.gov/Pages/ofpc/Index.aspx**](http://www.doa.la.gov/Pages/ofpc/Index.aspx) **. The application consists of six (6) pages. Two additional 8-1/2 x 11 inch pages may be included. These shall include any continuations of answers to questions on the application, additional information, etc. Applications in any other format will not be considered. Applications with more than a total of eight (8) 8-1/2 x 11 inch pages will not be accepted. One fully completed, signed and sealed copy of each application shall be submitted. The copy may be printed and mailed or printed and delivered or scanned in PDF format and e-mailed. Printed submittals shall not be bound or stapled. E-mailed PDF copies, as well as printed copies, shall be received by Facility Planning & Control within the deadline stated above. The date and time the e-mail is received in the Microsoft Outlook Inbox at Facility Planning & Control shall govern compliance with the deadline for e-mailed applications. Timely delivery by whatever means is strictly the responsibility of the applicant. By e-mailing an application the applicant assumes full responsibility for timely electronic delivery. DO NOT submit both printed and e-mail copies. Any application submitted by both means will be discarded.**   **1. Replacement of Wave Attenuators, Cypremort State Park, Cypremort Point, Louisiana, Project No. G06-264-16-ORM, Part 01.** The project consists of beach erosion protection at Cypremort State Park Beach. The storm surge from Hurricane Gustav on September 1, 2008 caused damage to the Wave Attenuator system located at Cypremort State Park. The remaining system components and anchor system have been removed. A new 1,274 lin. ft. erosion protection system inclusive of anchorage is to be designed approximately 200' from the shoreline. Funding for this project is provided, in part, by the Federal Emergency Management Agency and their participation and oversight may be expected in all phases of the project. The Designer shall prepare and submit all required drawings to Facility Planning and Control in AutoCAD. Drawings shall follow the format specified in the "Instructions to Designers for AutoCAD Drawings Submittal". The funds available for construction are approximately **$1,500,000.00** with a fee of approximately **$112,725.00**. Contract design time is **120** consecutive calendar days; including **30** days review time. Thereafter, liquidated damages in the amount of **$150.00** per day will be assessed. Further information is available from **Ms. Dawn Picard - Facility Planning and Control, Post Office Box 94095, Baton Rouge, Louisiana 70804-9095, (225) 219-1129.**   **2. Atchafalaya Basin Depth Restoration Project, Iberia Parish, Louisiana, Project No. 11-431-99-01, Part 81.** This project consists of dredging work in Grand Lake and Little Bayou Pigeon in the Atchafalaya Basin near the city of Jeanerette. The Grand Lake work consists of the removal of a large sand bar formed as a result of a breach in a nearby canal plug, and restoring the lake to a pre-breach bottom elevation. The Little Bayou Pigeon dredging will remove debris and sediment to improve the boat access in the bayou. The design and sediment placement will be in accordance with the US Army Corp of Engineers permit for this project, and the Designer will supply drawings to the Agency if an amendment to the permit is required. The Designer will be responsible for transportation to the site. The Designer’s fee has been adjusted to reflect the simplicity of the project and the ability to combine the design submittals. The Designer shall prepare and submit all required drawings to Facility Planning and Control in AutoCAD. Drawings shall follow the format specified in the "Instructions to Designers for AutoCAD Drawings Submittal". The funds available for construction are approximately **$1,500,000.00** with a fee of approximately **$106,094.00**. Contract design time is **90** consecutive calendar days; including **30** days review time. Thereafter, liquidated damages in the amount of **$125.00** per day will be assessed. Further information is available from **Mr. Creighton Stout - Facility Planning and Control, Post Office Box 94095, Baton Rouge, Louisiana 70804-9095, (225) 342-3378.**   **3. Fire Suppression System, LSU Frey Computer Center, Louisiana State University, Baton Rouge, Louisiana, Project No. 15-0383, Part 00.** This project consists of upgrades to existing fire suppression system. Designer is to specify all necessary parts and components for a complete, functioning, code compliant total flooding clean agent fire suppression system including a supplemental pre-action water suppression system in the machine room. All other areas of the building shall be protected with a combination of pre-action or wet fire sprinkler systems. Architectural services will be required to provide partition offices in the existing machine room service space and to provide for sprinkler rooms and closets as needed. The LSU Frey Computer Center is a 3 story, 4687 SF building that was built in 1996 and houses the University's computing systems. The function of the building will remain, and the project goal is to provide a higher standard of fire protection than the existing system currently provides. The Designer shall prepare and submit all required drawings to Facility Planning and Control in AutoCAD. Drawings shall follow the format specified in the "Instructions to Designers for AutoCAD Drawings Submittal". The funds available for construction are approximately **$700,000.00** with a fee of approximately **$75,676.00**. Contract design time is **180** consecutive calendar days; including **60** days review time. Thereafter, liquidated damages in the amount of **$100.00** per day will be assessed. Further information is available from **Mr. Roger Husser - Louisiana State University, Facility Services Building, Room 202, Baton Rouge, LA 70803, (225) 578-0803.**   **GENERAL REQUIREMENTS APPLICABLE TO ALL PROJECTS:** Applicants are advised that design time ends when the Documents are "complete, coordinated and **ready for bid**" as stated in to Article 3.3.1 4) of the Capital Improvements Projects Procedure Manual for Design and Construction. Documents will be considered to be "complete, coordinated and ready for bid" only if the advertisement for bid can be issued with no further corrections to the Documents. Design time will not necessarily end at the receipt of the initial Construction Documents Phase submittal by Facility Planning and Control. Any re-submittals required to complete the documents will be included in the design time.   In addition to the statutory requirements, professional liability insurance covering the work involved will be required in an amount specified in the following schedule. This will be required at the time the designer's contract is signed. Proof of coverage will be required at that time. **SCHEDULE LIMITS OF PROFESSIONAL LIABILITY**   |  |  |  | | --- | --- | --- | | Construction Cost |  | Limit of Liability | | $0 to $1,000,000 |  | $500,000 | | $1,000,000 to $10,000,000 |  | $1,000,000 | | $10,000,000 to $20,000,000 |  | $1,500,000 | | $20,000,000 to $50,000,000 |  | $3,000,000 | | Over $50,000,000 |  | To be determined |   Applicant firms should be familiar with the above stated requirements prior to application. The firm(s) selected for the project(s) will be required to sign the state's standard Contract Between Owner and Designer. When these projects are financed either partially or entirely with Bonds, the award of the contract is contingent upon the sale of bonds or the issuance of a line of credit by the State Bond Commission. The State shall incur no obligation to the engineer until the Contract Between Owner and Designer is fully executed.   Firms will be expected to have all the expertise necessary to provide all engineering services required by the Louisiana Capital Improvement Projects Procedure Manual for Design and Construction for the projects for which they are applying. Unless indicated otherwise in the project description, there will be no additional fee for consultants.   Facility Planning and Control is a participant in the Small Entrepreneurship Program (the Hudson Initiative) and applicants are encouraged to consider participation. Information is available from the Office of Facility Planning and Control or on its website at [www.doa.la.gov/Pages/ofpc/Index.aspx](http://www.doa.la.gov/Pages/ofpc/Index.aspx).   ANY PERSON REQUIRING SPECIAL ACCOMMODATIONS SHALL NOTIFY FACILITY PLANNING AND CONTROL OF THE TYPE(S) OF ACCOMMODATION REQUIRED NOT LESS THAN SEVEN (7) DAYS BEFORE THE SELECTION BOARD MEETING.   Applications shall be delivered or mailed to :   Applications shall be delivered or mailed or emailed to :  **LOUISIANA ENGINEERING SELECTION BOARD  c/o FACILITY PLANNING AND CONTROL**   |  |  |  |  |  | | --- | --- | --- | --- | --- | | |  | | --- | | **Deliver: 1201 North Third Street Claiborne Office Building Seventh Floor, Suite 7-160 Baton Rouge, LA 70802** | | |  | | --- | | **Mail: Post Office Box 94095 Baton Rouge, LA 70804-9095** | | **E-Mail: selection.board@la.gov** | |   **Use this e-mail address for applications only. Do not send any other communications to this address.**  The tentative meeting date for the Louisiana Engineering Selection Board is **Thursday, January 7, 2016 at 11:00 AM at Claiborne Building, 1201 N. Third Street, Room 1-153, Baton Rouge, Louisiana 70802.** |