**Scope of Work:**

Contractor shall furnish all labor, tools, equipment, & materials to create a new parking area at Raymond Laborde Correctional Center.

**Jobsite Location:**

Raymond Laborde Correctional Center

1630 Prison Road

Cottonport, LA 71327

**Job Specifications:**

\*Contractor shall strip topsoil (approximately 60’ X 100’ area). Topsoil shall be kept on facility grounds.

\*Contractor shall grade, level, and compact the soil.

\*Contractor shall place geotextile fabric & a minimum of 6” of crushed Portland Cement (or equal) in the graded area.

\*Contractor shall pour a minimum of 2” of asphalt over the newly prepared area (approximately 6350 square feet).

\*Contractor shall stripe the newly paved parking lot.

**Planning & Scheduling:**

* Before entering the facility grounds to commence work, Contractor shall check in with the maintenance department every day.
* Work hours shall be 7:30 AM to 3:30 PM, Monday through Friday, unless approved by the Maintenance Manager, James Desjardine

**Jobsite Visit Contact:**

James Desjardine james.desjardine@la.gov

Office - 318-876-4245

Cell - 318-305-8751

Josh Dauzat joshua.dauzat@la.gov

Office - 318-876-4246

Cell - 318-305-0955