**Scope of Work:**

The Contractor shall provide all labor and materials in order to install approximately 700’ of three board white vinyl fence and one double gate at the Southwest Louisiana Veterans Cemetery for the Louisiana Department of Veterans Affairs (DVA).

**Location:**

Southwest Louisiana Veterans Cemetery

1620 Evangeline Hwy

Jennings, LA 70564

**Specifications:**

* The Contractor shall remove the existing barbed wire fence on the north side of the Cemetery property along Interstate 10. The newly installed fence shall replace existing fence.
* The new fence shall be constructed of white vinyl boards that shall match the current fence on the south side of the Cemetery (see Attachment D).
* The fence posts shall be 5” x 5” cemented into the ground so the height of the post cap shall be approximately 52” from the ground. The distance from each post shall be approximately 95” apart from center to center or approximately 91 ½” from inside to inside. Each fence post shall have a cap.
* The rails shall be 16’ x 5 ½” x 1 ½”, spaced approximately 11 ½” apart.
* The double gate shall be constructed of two 4’ gates in order to provide an 8’ opening.
* The fence shall be constructed to meet all wind rating codes.

**Terms and Conditions:**

* All labor, equipment, materials, and delivery in accordance with the scope of work.
* The Contractor shall work cleanly, safely and securely.
* The Contractor shall remove all packing and debris from facility created during the job.
* The Contractor shall comply with all state and federal laws and regulations.
* The Contractor shall obtain any necessary permits, be licensed and insured.
* Mandatory Job-Site Visit. Schedule appointments with Dwayne Guidry 337-246-7094, Monday-Friday 8am – 3pm.