**Specifications for replacement of VCT Flooring and Cove Base**

**Louisiana Secretary of State Archives Building**

**Scope of Work:**

The Contractor shall provide all labor and materials in order to remove, dispose, and replace VCT Flooring and Cove Base for the Louisiana Secretary of State (SOS).

**Location:**

Secretary of State Archives Building

3851 Essen Lane

Baton Rouge, Louisiana 70809

**Description:**

* The Contractor shall remove and dispose of the existing floor and baseboard.
* The Contractor shall provide and install new Cove Base (approximately 1,800 Linear Ft.)
  + Roppe Cove Base 4” 700 series 1/8” Black or equal
  + 4’ lengths
  + Mapei 575 Cove Base Adhesive- Mapei 575 Cove base Adhesive 28oz tube or equal
* The Contractor shall provide and install VCT (approximately 9,900 Sq. Ft.).
  + Tarkett VCT II 12X12 or equal
  + Mapei Eco 711 4 Gal VCT Adhseive or equal
* The Contractor shall prep the newly installed floor for waxing and buffing.
* After installation is complete, the Contractor shall Wax and Buff the newly installed flooring.

**Terms and Conditions:**

* All work being performed shall be required during normal business hours. Monday through Friday 8:00am to 4:30pm unless otherwise approved.
* All waste/debris shall be removed from the site daily and disposed of properly by the Contractor.