**Scope of Work**

The Contractor shall provide all labor and materials in order to provide and install a Intrex Innovative Solutions Rythmos System for the Louisiana Department of Veterans Affairs (DVA).

**Location:**

Louisiana Veterans Home

4739 Hwy 10

Jackson, LA 70748

**\*\*\*In accordance with La R.S. 39:1655, this solicitation has been approved as proprietary, and only the brands and models specified will be considered for award.\*\*\***

The Contractor shall provide and install a new Intrex Innovative Solutions Rythmos System to be installed for comprehensive senior risk management of residents in senior communities (i.e. Nursing Homes) in order to provide personalized support and guidance to caregivers and residents. The system shall be installed by a licensed and certified distributor of Intrex Innovative Solutions Rythmos Systems for proper integration.

**Specifications:**

System shall include a minimum of:

* Two Gateways
* 150 Beacons
* Fall detection
* 60 Access Control Readers
* 30 Remote Keyswitch
* 40 Mag Lock with Bracket
* 12 Remote Release
* 10 Community and Wearable Rechargeable Bracelet/Necklace
* 100 Employee Fobs (or alternate based on agency preference and discretion)
* Two Community five Port Dock Stations
* One Community Swap Pad
* 20 Community Locking Bands
* Six 32” Nurse Station Monitoring Consoles
* Annual Cloud and Software Maintenance
* ProActive Monitoring for 30 Patient Wandering doors with Access Control

\*All Fire wall penetrations made that day must be repaired by the Contractor before leaving that day.

\*All Fire Stop material must be approved by the Maintenance Supervisor and in accordance with Fire Life Safety Standards before using.

\*The MSDS 'SDS' sheet must be provided by the Contractor to the Maintenance Department before usage of the material.

\*All Fire Wall penetrations must be inspected by the Maintenance Supervisor before the ceiling tile(s) are able to be put back in place.