**Scope of Work**

The Contractor shall furnish all necessary labor, materials, tools, equipment, and supervision to remove and replace the current freezer & cooler doors for the Louisiana Department of Correction (DOC).

**Location:**

DOC Allen Correctional Center

3751 Lauderdale Woodyard

Kinder, LA 70648

**Site Visit Contact:**

Taylor Maricle

337-375-6611

Taylor.Maricle@la.gov

**Specifications:**

* Two freezer and three cooler doors shall be replaced and installed by the Contractor.
* The Contractor shall install custom built doors.
* The doors must meet the following standards of performance:
  + 4-5 inches of insulation
  + Able to withstand temperatures of -10 degrees Fahrenheit.
  + If the doors must be hard wired in, the Agency will do that themselves.
  + No windows are needed on doors.
  + A regular pull handle will suffice, there is currently a latch on the top of each door.
  + All doors will need to lock.
* Each freezer/cooler has a single door.
* Door sizes are:

Cooler M= 36 ½ w x 78 ½ h

Cooler D= 36 ½ w x 78 ½ h

Cooler B= 35 ¼ w x 77 ½ h

Freezer F= 35 ¼ w x 77 ½ h

Freezer A= 35 ¼ w x 77 ½ h

**General Terms:**

* The Contractor shall be responsible for delivery and pickup of materials/supplies needed to complete project.
* Disposal of all materials, and debris shall be the responsibility of the Contractor.
* The Contractor is responsible for removing and disposing of the old doors.