**Scope of Work:**

The Contractor shall construct, install, and replace Treatment Plant Equipment and Grating for the Louisiana Department of Corrections (DOC).

**Location:**

Dixon Correctional Institute

5568 Highway 68

Jackson LA 70748

**Site Visit Contact:**

Will Bunch

225-634-6101

**Specifications:**

* The Contractor shall construct and install new stainless steel bar screen and bolt it down to the concrete and hook force main to the bar screen.
* The Contractor shall construct and install new stainless steel weir through for clarifier.
* The Contractor shall construct and install new sludge returns and skimmers in clarifier.
* The Contractor shall construct and install new stainless steel air header from blower’s aeration.
* The Contractor shall construct and install new stainless steel air drops with find bubble diffusers and valves along with necessary pipping and metals.
* The Contractor shall install new duplex blower system complete with sound dampening enclosure and control panel.
* The Contractor shall replace all metal grating on treatment plant.
* The Contractor shall replace influent pump station pumps, rails, base elbows, floats, valves, aeration system, and control panel.

**General Terms and Conditions:**

* Warranty if applicable
* Work shall be performed Monday-Friday from 7:00 am – 3:30 pm.
* The Contractor’s representatives are subject to a search of their vehicles, possessions and persons. This is necessary to preclude the introduction of weapons, ammunition, explosives, cell phones, alcohol, escape devices, drugs and drug paraphernalia or other forbidden items or contraband into the prison environment. All searches of visitors will be conducted in accordance with Department Regulation No. C-02-005 and Penitentiary Directive No. 09.004 and 09.004A.
* The Contractor’s representatives are subject to a background check.
* The Contractor’s representatives must follow all institutional policies and procedures while performing work on facility grounds.
* The Contractor is subject to a conference/training with facility staff after the contract is executed and before performing any work.
* Disposal of all materials, and debris shall be the responsibility of the Contractor.