Brand: Epilog or Equal

Model: Fusion Pro 24 Combo or Equal

Specifications and Accessories:

Minimum Work Space Dimensions: 24” x 24”

* Machine must be dual source and include: CO2 Laser – Air cooled, metal/ceramic waveguide tube, 10.6 micrometers
  + 60 Watts
* Fiber – Air cooled, includes collimator, 1065 nm beam quality: M2<1.1
  + 30 Watts
* IRIS or Equal Camera System
* 2” CO2 Lens and 3” Fiber and Dual Source Lens
* Print Driver & Software – Laser Dashboard and Epilog or Equal Job Manager
* Vector Cutting Table (Grid Style)
* Air Assist Compressor/Pump
* Fusion Pro or Equal Rim-Style Rotary Attachment
* Accessory Relay Unit
* 4” CO2 Lens
* Onsite Training for Two Employees
* Customer Service Access for Trouble Shooting