**Attachment C –**

**Specifications**

**RFx 3000024597**

**Scope of Work:**

The Contractor shall furnish all labor, materials, tools and equipment necessary to install backflow prevention system to bring domestic and fire water system up to code for the Louisiana Department of State (DOS).

**Location:**

3851 Essen Lane

Baton Rouge, La. 70809

**Site Visit Contact:**

James Bunch

225-922-2047

**Specifications:**

* The Contractor shall install a new 6” double check-detector backflow prevention assembly (DCDA) for Fire System.
* The Contractor shall install a new 3” DCDA for domestic water.
* The Contractor shall construct a Hazard Custom Hot Box Enclosure to house both Backflows to prevent the pipes from freezing. The Contractor shall obtain measurements during the mandatory jobsite visit.
* The custom color must be Stone White to match the exterior walls of the property.

**Terms and Conditions:**

* All corrections for work that is unsatisfactory shall be corrected at the Contractor’s expense and shall be completed satisfactorily before approval and final payment can be made.
* Work hours shall take place from 8:00 A.M. to 4:30 PM – Monday through Friday unless otherwise approved.
* All waste/debris shall be removed from the site daily and disposed of properly by the Contractor.