**Scope of Work:**

The Contractor shall supply all labor, equipment, supplies, and materials to build and install awning cover for the Louisiana Department of Public Safety (DPS).

**Location:**

Louisiana State Police  
Troop B  
2101 I-10 Service Rd  
Kenner, LA 70065

**Site Visit Contact:**

Sgt. Robert Goertz

(504) 471-2775 or (504) 650-1319

**Specifications**

* The Contractor shall construct lean-to awning over 40’ container to create dry area.
* The materials used for this project shall be commercial grade steel and solid concrete footings.
* The awning shall extend from the wall out to 20’ and the length of the awning shall be approximately 49’.
* The height of the awning at the building shall be at 10’ and shall have a fall of 4” to end at 9’6”.
* There shall be a 2’ fascia added as requested.
* The materials used shall be 11-guage steel.
* The post shall be 4 x 4 x 1/4” and steel Z purlins for the R panel roof.
* The awning shall be a single bay free standing structure but will be tied to building for added support.

**General Terms and Conditions:**

* All corrections for work that is unsatisfactory shall be corrected at the Contractor’s expense and must be completed satisfactorily before approval and final payment is made.
* The Contractor shall be responsible for removal of any and all waste material generated by this project.
* No electricity shall be installed on this project.
* The project shall include one year of workmanship warranty.