**Installation of a Three Sided Metal Building with Open Front**

**Location:**

Louisiana Department of Wildlife and Fisheries

Pineville Field Office

1995 Shreveport Hwy 71 North

Pineville, LA 71360

**Scope of Work:**

To furnish all labor, materials, tools, equipment, and supplies necessary to install one, three sided metal building, with an open front.

**Requirements:**

* Install a 70' x 24' x12' tall metal building on an existing concrete slab.
* The building shall slopes from 12' to 10' in height, from front to back. Three sides walled, with the front open.
* To have a bolted frame construction.
* Posts to be attached to concrete with 1/2" bolts.
* To have 4" x 4", 14 gauge steel posts.
* Wall girts to be 4" Cee, 14 gauge steel at 4' spacing, bottom wall girt raised off slab 2".
* Roof purlins to be 10" Cee, 14 gauge steel, spaced 4'.
* Channel to be 10" Cee, 14 gauge steel.
* Install brace supports for 35' span.
* Metal roof panels to be R panel, 26 gauge. Metal roof panels to be the color green.
* Metal trim to be 26 gauge. Metal trim to be the color green.
* Metal wall panels to be 26 gauge. Metal wall panels to be the color tan.
* All waste generated from project is to be removed by the Contractor. A dumpster will not be provided.