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October 13, 2026

Addendum No. 03 

Your reference is directed to RFx Number 300002663 for the Invitation to Bid (ITB) for the State of Louisiana – Tower Removal - LDAF, which is currently scheduled to open at 10:00 AM CT on 10/20/2026.

The following are the Vendor’s Inquiries received by the deadline date of September 22, 2026, and the State’s Responses:

Vendor’s Inquiry #1: When do you expect the radio tower to be removed? 

State’s Response #1: The Contractor must provide their estimated time of completion for the project with their bid submission.

Vendor’s Inquiry #2: How tall is this tower?   

State’s Response #2: 110 feet

Vendor’s Inquiry #3: Can the tower be tipped (like a tree?)

State’s Response #3: The method of demolition is at the Contractor’s discretion; however, all tower parts must remain on the landowner’s property when the tower is dropped.

Vendor’s Inquiry #4: Is the foundation pier removal required? Do you have foundation prints? How deep do they go? How wide are they at the base? 

State’s Response #4: Everything at the location of the tower, including the foundation, must be removed. The piers are pyramid-shaped and are on average approximately 2 feet at the top, 5 feet at the bottom, and 8 feet tall. There are no prints or specifications available.

Vendor’s Inquiry #5: Are there overhead or underground utilities that must be disconnected or protected?

State’s Response #5: Everything at the site should be disconnected. A site visit must be performed to identify.

Vendor’s Inquiry #6: Are there any hazardous materials or hazardous coatings associated with the tower that bidders should account for?

State’s Response #6: The tower is coated with galvanized steel.

Vendor’s Inquiry #7: Is there an existing drawing, survey, or specification showing the tower dimensions, structural members, platform, and foundation layout?

State’s Response #7: There are no specifications available for the tower. A site visit is recommended to become familiar with the tower.

Vendor’s Inquiry #8: Approximately how much does the tower and associated steel weigh?

State’s Response #8: There are no specifications available for the tower. A site visit is recommended to become familiar with the tower.

Vendor’s Inquiry #9: Can the Contractor bring in excavators, skid steers, cranes, dump trucks, or other heavy equipment needed for the demolition?

State’s Response #9: Yes.

Vendor’s Inquiry #10: Are there any restrictions on clearing or trimming vegetation to provide equipment access?

State’s Response #10: No. 

Vendor’s Inquiry #11: Will LDAF provide utility locations, surveys, or utility marking prior to demolition?

State’s Response #11: Reaching out to Louisiana 811 will be the responsibility of the awarded Contractor.

Vendor’s Inquiry #12: Is the tower connected to any electrical, communications, security, or other utilities that must be disconnected by the Contractor?

State’s Response #12: No

Vendor’s Inquiry #13: Are there any known underground tanks, lines, drainage structures, or other site improvements in the work area?

State’s Response #13: Yes, a site visit must be performed to identify.

Vendor’s Inquiry #14: Are there any materials that LDAF wants salvaged and returned to the agency rather than disposed of?

State’s Response #14: No, everything must be removed and disposed of.

Vendor’s Inquiry #15: Should the excavated concrete/foundation material be replaced with imported fill, or may suitable excavated soil be reused?

State’s Response #15: Suitable excavated soil can be reused. There is not a specific dirt or soil required.

Vendor’s Inquiry #16: Is the Contractor required to submit a demolition plan, safety plan, or equipment plan before beginning work?

State’s Response #16: Yes. 

Vendor’s Inquiry #17: Are there restrictions on cutting or dropping tower sections during demolition?

State’s Response #17: See response to vendor inquiry #3.

Vendor’s Inquiry #18: What type of foundation exists below grade?

State’s Response #18: Concrete foundation

Vendor’s Inquiry #19: If complete foundation removal is required and the below-grade foundation configuration, dimensions, or construction cannot reasonably be determined before excavation, how will unforeseen subsurface conditions and any resulting additional work or cost be addressed under the contract?

State’s Response #19: Unforeseen subsurface conditions and additional work will be addressed by change orders.

Vendor’s Inquiry #20: What is the minimum required depth of foundation removal below grade?

State’s Response #20: The foundation must be completely removed, there is no minimum required depth. 

Vendor’s Inquiry #21: What type of backfill material is required?

State’s Response #21: See response to vendor inquiry #15.

Vendor’s Inquiry #22: Is a compaction test of the backfill soil required?

State’s Response #22: No.
Vendor’s Inquiry #23: Are there any prohibited tools, equipment, or demolition methods?

State’s Response #23: No.

Vendor’s Inquiry #24: Are there any specialized PPE requirements for this project?

State’s Response #24: This should be determined by the awarded Contractor.

Vendor’s Inquiry #25: Are there any prohibited types or weight classes of vehicles or equipment allowed on the site?

State’s Response #25: No.

Vendor’s Inquiry #26: Are there any special precautions or requirements for protecting the access road due to its current poor condition?

State’s Response #26: The bridges and roads must be in the same shape as they were when the project began.

Vendor’s Inquiry #27: May vegetation or shrubs on the natural land near the tower be trimmed as necessary to provide equipment and personnel access? 

State’s Response #27: Yes.


All else remains as on original Invitation to Bid.


This addendum is hereby officially made a part of the referenced solicitation. 
Acknowledgement: If you have already submitted your bid and this Addendum does not cause you to revise your bid, you should acknowledge receipt of this Addendum by identifying your business name and by signing where indicated.  You may return this Acknowledgement by mail or delivery by hand or courier to: Office of State Procurement, 1201 N. 3rd Street, Ste. 2-160, Baton Rouge, LA  70802, or by fax to: (225) 342-9756.  The State reserves the right to request a completed Acknowledgement at any time.  Failure to execute an Acknowledgement shall not relieve the bidder from complying with the terms of its bid.
Addendum Acknowledged/No changes:

For:  ________________________  By:  __________________________





Revision: If you have already submitted your bid and this Addendum requires you to revise your bid, you must indicate any change(s) below, identify your business name and sign where shown.  Revisions shall be delivered prior to bid opening by mail or delivery by hand or courier to: Office of State Procurement, 1201 N. 3rd Street, Ste. 2-160, Baton Rouge, LA  70802, or by fax to: (225) 342-9756, and indicate the RFx number and the bid opening date and time on the outside of the envelope for proper identification.  Electronic transmissions other than by fax are not being accepted at this time.


Revisions received after bid opening shall not be considered and you shall be held to your original bid.

Revision:

For:  ________________________  By:  __________________________


By:	Arkeith White
	Office of State Procurement
	Telephone No. 225-219-4207
	Email:  Arkeith.white@la.gov
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