


Attachment C – Scope of Work and Specifications
RFx 3000026790

**If bidding other than specified, please provide manufacturer’s specs for “or equal” items. **

Scope of Work:
The Contractor shall provide all labor, equipment, and materials needed to remove and replace approximately 6,000 sq. ft. of roofing for the Louisiana Department of Health (LDH).

Site Visit Contact:
[bookmark: _Hlk241818890]Shannon Aymond, (318) 641-2286

Location:
Pinecrest Supports and Service Center
884 Pinecrest Dr. 
Pineville, la. 71360
Specifications: 
The Contractor shall provide the following:
· Remove the existing roof membrane down to gypsum decking.

· Install a new Permaply 28 or Equal base sheet over gypsum decking and anchor with Ultralok or Equal fasteners. 

Specify Base Sheet Bidding: _____________

Specify Fasteners Bidding: ______________
· Install new polyiso tapered system sloped to a ¼" fall to perimeter edges of roof. The taper shall have a 1-1/2" minimum start.
· Adhere tapered system with UIA adhesive or equal.

Specify Adhesive Bidding: _____________

· Install new ½" Dexcell FA or Equal cover board over the tapered insulation and adhere with UIA adhesive or equivalent.

Specify Roofing Cover Board Bidding: _____________

Specify Adhesive Bidding: _____________

· Install new 60 mil TPO membrane over Dexcell FA or Equal cover board and adhere with adhesive thoroughly.

Specify Roofing Cover Board Bidding: _____________
· Install any related curb flashings
· Install any related wood blocking around perimeter edge.


General Terms and Conditions:
· The Contractor shall provide a dumpster and ensure all debris is cleaned from the ground around site daily.
· The job must include two years of workmanship warranty and a 20-year Manufacturers NDL Warranty
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