Attachment B – Specifications

RFx 3000026770	
FirstWatch PFD Gear - LDWF

FirstWatch 40PROA Law Enforcement Personal Floatation Device
· USCG Approved- UL1180- Inflatable PFDs Type 5 (Commercial Use); Type II (Recreational Use)
· 40 Pounds of Buoyancy (38 Gram CO2)
· High Visibility Yellow Inflatable Cell, with Reflective Tape.
· Automatic HRC l-F Hydro V95000 Compact Inflator
· 1-F Single Point Inflator Status Indicator Green
· Universal Sizing
· Secure Pull for Inflation
· Zipper Opens Upon Inflation; Easy to Repack
· 1.5" Nylon Webbing with Dual Adjustment (Right and Left), Anti-Abrasion Rib Pads
· Molded Foam and Mesh Construction for Comfort and Vapor Management
· Designed to Ease Pressure Points Behind Neck
· Right Side Small Zip Enclosure Accessory Pocket
· Internal Spare Pouch for Co2 inflator re-arm kit
· Radio Mic Loops on Right and Left Breast
· Wide Chest Spacing to Accommodate Body Worn Camera
· Ultra Strong 2" Nylon Webbing Waist Belt Expands to a Chest Width of 56"

Automatic Inflatable Re-arm Kit SA V95000-86202Z Re-arm Kit
· Must Include 38 Gram CO2 Cartridge
· UL Approved Marine
· Cartridge is ½" threaded
· Must include 1 Halkey-Roberts V80040 Yellow Bobbin
· Must include 1 Halkey-Roberts V85006 Green Indicator Pin
· Must be Compatible with First Watch 40PROA Law Enforcement PFD
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